# RadioLib: src/modules/SX126x/SX1262.h Source File

SX1262.h
#if !defined(_RADIOLIB_SX1262_H)
#define _RADIOLIB_SX1262_H
#include "../../TypeDef.h"
#if !RADIOLIB_EXCLUDE_SX126X
#include "../../Module.h"
#include "SX126x.h"
//RADIOLIB_SX126X_CMD_SET_PA_CONFIG
#define RADIOLIB_SX126X_PA_CONFIG_SX1262 0x00
//RADIOLIB_SX126X_REG_VERSION_STRING
// Note: this should really be "2", however, it seems that all SX1262 devices report as SX1261
#define RADIOLIB_SX1262_CHIP_TYPE "SX1261"
class SX1262: public SX126x {
public:
SX1262(Module* mod); // cppcheck-suppress noExplicitConstructor
// basic methods
int16_t begin(float freq = 434.0, float bw = 125.0, uint8_t sf = 9, uint8_t cr = 7, uint8_t syncWord = RADIOLIB_SX126X_SYNC_WORD_PRIVATE, int8_t power = 10, uint16_t preambleLength = 8, float tcxoVoltage = 1.6, bool useRegulatorLDO = false);
int16_t beginFSK(float freq = 434.0, float br = 4.8, float freqDev = 5.0, float rxBw = 156.2, int8_t power = 10, uint16_t preambleLength = 16, float tcxoVoltage = 1.6, bool useRegulatorLDO = false);
// configuration methods
int16_t setFrequency(float freq) override;
int16_t setFrequency(float freq, bool calibrate);
virtual int16_t setOutputPower(int8_t power) override;
int16_t checkOutputPower(int8_t power, int8_t* clipped) override;
#if !RADIOLIB_GODMODE
private:
#endif
};
#endif
#endif
Module
Implements all common low-level methods to control the wireless module. Every module class contains o...
Definition: Module.h:65
SX1262
Derived class for SX1262 modules.
Definition: SX1262.h:22
SX1262::SX1262
SX1262(Module *mod)
Default constructor.
Definition: SX1262.cpp:4
SX1262::setFrequency
int16_t setFrequency(float freq) override
Sets carrier frequency. Allowed values are in range from 150.0 to 960.0 MHz.
Definition: SX1262.cpp:50
SX1262::checkOutputPower
int16_t checkOutputPower(int8_t power, int8_t *clipped) override
Check if output power is configurable.
Definition: SX1262.cpp:122
SX1262::beginFSK
int16_t beginFSK(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=156.2, int8_t power=10, uint16_t preambleLength=16, float tcxoVoltage=1.6, bool useRegulatorLDO=false)
Initialization method for FSK modem.
Definition: SX1262.cpp:32
SX1262::begin
int16_t begin(float freq=434.0, float bw=125.0, uint8_t sf=9, uint8_t cr=7, uint8_t syncWord=RADIOLIB_SX126X_SYNC_WORD_PRIVATE, int8_t power=10, uint16_t preambleLength=8, float tcxoVoltage=1.6, bool useRegulatorLDO=false)
Initialization method for LoRa modem.
Definition: SX1262.cpp:8
SX1262::setOutputPower
virtual int16_t setOutputPower(int8_t power) override
Sets output power. Allowed values are in range from -9 to 22 dBm. This method is virtual to allow ove...
Definition: SX1262.cpp:100
SX126x
Base class for SX126x series. All derived classes for SX126x (e.g. SX1262 or SX1268) inherit from thi...
Definition: SX126x.h:443