# RadioLib: src/protocols/Print/Print.h Source File

Print.h
#if !defined(_RADIOLIB_PRINT_H)
#define _RADIOLIB_PRINT_H
#include <string.h>
#include "ITA2String.h"
// supported encoding schemes
#define RADIOLIB_ASCII 0
#define RADIOLIB_ASCII_EXTENDED 1
#define RADIOLIB_ITA2 2
class RadioLibPrint {
public:
virtual size_t write(uint8_t) = 0;
size_t write(const char *str) {
if (str == NULL) return 0;
return write(reinterpret_cast<const uint8_t *>(str), strlen(str));
}
virtual size_t write(const uint8_t *buffer, size_t size);
size_t write(const char *buffer, size_t size) {
return write(reinterpret_cast<const uint8_t *>(buffer), size);
}
size_t print(ITA2String& ita2);
size_t println(ITA2String& ita2);
#if defined(RADIOLIB_BUILD_ARDUINO)
size_t print(const __FlashStringHelper *);
size_t print(const String &);
size_t println(const __FlashStringHelper *);
size_t println(const String &);
#endif
size_t print(const char[]);
size_t print(char);
size_t print(unsigned char, int = DEC);
size_t print(int, int = DEC);
size_t print(unsigned int, int = DEC);
size_t print(long, int = DEC);
size_t print(unsigned long, int = DEC);
size_t print(double, int = 2);
size_t println(const char[]);
size_t println(char);
size_t println(unsigned char, int = DEC);
size_t println(int, int = DEC);
size_t println(unsigned int, int = DEC);
size_t println(long, int = DEC);
size_t println(unsigned long, int = DEC);
size_t println(double, int = 2);
size_t println(void);
#if !RADIOLIB_GODMODE
protected:
#endif
uint8_t encoding = RADIOLIB_ASCII_EXTENDED;
const char* lineFeed = "\r\n";
size_t printNumber(unsigned long, uint8_t);
size_t printFloat(double, uint8_t);
};
#endif
ITA2String
ITA2-encoded string.
Definition: ITA2String.h:24
RadioLibPrint
Printing class, based on Arduino Print class with additional encodings.
Definition: Print.h:17