# RadioLib: Member List

SX1231 Member List

This is the complete list of members for SX1231, including all inherited members.

available() | PhysicalLayer |
begin(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=125.0, int8_t power=10, uint8_t preambleLen=16) | SX1231 |
calculateRxTimeout(RadioLibTime_t timeoutUs) | PhysicalLayer | virtual
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkOutputPower(int8_t power, int8_t *clipped) | PhysicalLayer | virtual
clearChannelScanAction() | PhysicalLayer | virtual
clearDio0Action() | RF69 |
clearDio1Action() | RF69 |
clearFifoEmptyAction() | RF69 |
clearFifoFullAction() | RF69 |
clearPacketReceivedAction() override | RF69 | virtual
clearPacketSentAction() override | RF69 | virtual
disableAddressFiltering() | RF69 |
disableAES() | RF69 |
disableContinuousModeBitSync() | RF69 |
disableSyncWordFiltering() | RF69 |
dropSync() | PhysicalLayer |
enableAES() | RF69 |
enableContinuousModeBitSync() | RF69 |
enableSyncWordFiltering(uint8_t maxErrBits=0) | RF69 |
fifoAdd(uint8_t *data, int totalLen, int *remLen) | RF69 |
fifoGet(volatile uint8_t *data, int totalLen, volatile int *rcvLen) | RF69 |
finishTransmit() override | RF69 | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_RF69_MAX_PACKET_LENGTH) | RF69 |
getChannelScanResult() | PhysicalLayer | virtual
getChipVersion() | RF69 |
getFreqStep() const | PhysicalLayer |
getFrequency(float *freq) | RF69 |
getFrequencyDeviation(float *freqDev) | RF69 |
getPacketLength(bool update=true) override | RF69 | virtual
getRSSI() override | RF69 | virtual
getSNR() | PhysicalLayer | virtual
getTemperature() | RF69 |
getTimeOnAir(size_t len) | PhysicalLayer | virtual
invertIQ(bool enable) | PhysicalLayer | virtual
irqRxDoneRxTimeout(uint32_t &irqFlags, uint32_t &irqMask) | PhysicalLayer | virtual
isRxTimeout() | PhysicalLayer | virtual
packetMode() | RF69 |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | RF69 | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | RF69 | virtual
readData(uint8_t *data, size_t len) override | RF69 | virtual
readData(uint8_t *data, size_t len) | RF69 |
receive(uint8_t *data, size_t len) override | RF69 | virtual
receive(uint8_t *data, size_t len) | RF69 |
receiveDirect() override | RF69 | virtual
reset() | RF69 |
RF69(Module *module) | RF69 |
scanChannel() | PhysicalLayer | virtual
setAESKey(uint8_t *key) | RF69 |
setAmbientTemperature(int16_t tempAmbient) | RF69 |
setBitRate(float br) override | RF69 | virtual
setBroadcastAddress(uint8_t broadAddr) | RF69 |
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setCrcFiltering(bool crcOn=true) | RF69 |
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) override | RF69 | virtual
setDio0Action(void(*func)(void)) | RF69 |
setDio1Action(void(*func)(void)) | RF69 |
setDIOMapping(uint32_t pin, uint32_t value) override | RF69 | virtual
setDirectAction(void(*func)(void)) override | RF69 | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | RF69 | virtual
setFifoEmptyAction(void(*func)(void)) | RF69 |
setFifoFullAction(void(*func)(void)) | RF69 |
setFrequency(float freq) override | RF69 | virtual
setFrequencyDeviation(float freqDev) override | RF69 | virtual
setLnaTestBoost(bool value) | RF69 |
setNodeAddress(uint8_t nodeAddr) | RF69 |
setOOK(bool enable) | RF69 |
setOokFixedThreshold(uint8_t value) | RF69 |
setOokPeakThresholdDecrement(uint8_t value) | RF69 |
setOokThresholdType(uint8_t type) | RF69 |
setOutputPower(int8_t pwr, bool highPower=false) | RF69 |
PhysicalLayer::setOutputPower(int8_t power) | PhysicalLayer | virtual
setPacketReceivedAction(void(*func)(void)) override | RF69 | virtual
setPacketSentAction(void(*func)(void)) override | RF69 | virtual
setPreambleLength(uint8_t preambleLen) | RF69 |
PhysicalLayer::setPreambleLength(size_t len) | PhysicalLayer | virtual
setPromiscuousMode(bool enable=true) | RF69 |
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | RF69 |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | RF69 |
setRSSIThreshold(float dbm) | RF69 |
setRxBandwidth(float rxBw) | RF69 |
setSyncWord(uint8_t *syncWord, size_t len, uint8_t maxErrBits=0) | RF69 |
PhysicalLayer::setSyncWord(uint8_t *sync, size_t len) | PhysicalLayer | virtual
sleep() override | RF69 | virtual
standby() override | RF69 | virtual
standby(uint8_t mode) override | RF69 | virtual
startChannelScan() | PhysicalLayer | virtual
startDirect() | PhysicalLayer |
startReceive() override | RF69 | virtual
startReceive(uint32_t timeout, uint32_t irqFlags, uint32_t irqMask, size_t len) override | RF69 | virtual
startTransmit(uint8_t *data, size_t len, uint8_t addr=0) override | RF69 | virtual
startTransmit(const char *str, uint8_t addr=0) | RF69 |
startTransmit(uint8_t *data, size_t len, uint8_t addr=0) | RF69 |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
SX1231(Module *mod) | SX1231 |
transmit(uint8_t *data, size_t len, uint8_t addr=0) override | RF69 | virtual
transmit(const char *str, uint8_t addr=0) | RF69 |
transmit(uint8_t *data, size_t len, uint8_t addr=0) | RF69 |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | RF69 | virtual
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_RF69_MAX_PACKET_LENGTH) | RF69 |