# RadioLib: src/modules/Si443x/Si4432.h Source File

Si4432.h
#if !defined(_RADIOLIB_SI4432_H)
#define _RADIOLIB_SI4432_H
#include "../../TypeDef.h"
#if !RADIOLIB_EXCLUDE_SI443X
#include "../../Module.h"
#include "Si443x.h"
class Si4432: public Si443x {
public:
// constructor
Si4432(Module* mod); // cppcheck-suppress noExplicitConstructor
// basic methods
int16_t begin(float freq = 434.0, float br = 4.8, float freqDev = 5.0, float rxBw = 181.1, int8_t power = 10, uint8_t preambleLen = 16);
// configuration methods
int16_t setFrequency(float freq) override;
int16_t setOutputPower(int8_t power) override;
#if !RADIOLIB_GODMODE
protected:
#endif
#if !RADIOLIB_GODMODE
private:
#endif
};
#endif
#endif
Module
Implements all common low-level methods to control the wireless module. Every module class contains o...
Definition: Module.h:65
Si4432
Derived class for Si4432 modules.
Definition: Si4432.h:15
Si4432::setOutputPower
int16_t setOutputPower(int8_t power) override
Sets output power. Allowed values range from -1 to 20 dBm in 3 dBm steps.
Definition: Si4432.cpp:31
Si4432::begin
int16_t begin(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=181.1, int8_t power=10, uint8_t preambleLen=16)
Initialization method. Must be called at least once from Arduino sketch to initialize the module.
Definition: Si4432.cpp:8
Si4432::setFrequency
int16_t setFrequency(float freq) override
Sets carrier frequency. Allowed values range from 240.0 MHz to 930.0 MHz.
Definition: Si4432.cpp:24
Si4432::Si4432
Si4432(Module *mod)
Default constructor.
Definition: Si4432.cpp:4
Si443x
Base class for Si443x series. All derived classes for Si443x (e.g. Si4431 or Si4432) inherit from thi...
Definition: Si443x.h:553