# RadioLib: Member List

nRF24 Member List

This is the complete list of members for nRF24, including all inherited members.

available() | PhysicalLayer |
begin(int16_t freq=RADIOLIB_NRF24_DEFAULT_FREQ, int16_t dr=RADIOLIB_NRF24_DEFAULT_DR, int8_t pwr=RADIOLIB_NRF24_DEFAULT_POWER, uint8_t addrWidth=RADIOLIB_NRF24_DEFAULT_ADDRWIDTH) | nRF24 |
clearIrqAction() | nRF24 |
clearPacketReceivedAction() | nRF24 | virtual
clearPacketSentAction() | nRF24 | virtual
disablePipe(uint8_t pipeNum) | nRF24 |
dropSync() | PhysicalLayer |
finishTransmit() override | nRF24 | virtual
getFreqStep() const | PhysicalLayer |
getMod() (defined in nRF24) | nRF24 | virtual
getPacketLength(bool update=true) override | nRF24 | virtual
getRSSI() | PhysicalLayer | virtual
getSNR() | PhysicalLayer | virtual
getStatus(uint8_t mask=0xFF) | nRF24 |
invertIQ(bool enable) | PhysicalLayer | virtual
isCarrierDetected() | nRF24 |
nRF24(Module *mod) | nRF24 |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() | PhysicalLayer | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) | PhysicalLayer | virtual
readData(uint8_t *data, size_t len) override | nRF24 | virtual
readData(uint8_t *data, size_t len) | nRF24 |
receive(uint8_t *data, size_t len) override | nRF24 | virtual
receive(uint8_t *data, size_t len) | nRF24 |
receiveDirect() override | nRF24 | virtual
setAddressWidth(uint8_t addrWidth) | nRF24 |
setAutoAck(bool autoAckOn=true) | nRF24 |
setAutoAck(uint8_t pipeNum, bool autoAckOn) | nRF24 |
setBitRate(float br) | nRF24 | virtual
setCrcFiltering(bool crcOn=true) | nRF24 |
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) override | nRF24 | virtual
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) | PhysicalLayer | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | nRF24 | virtual
setFrequency(float freq) | nRF24 | virtual
setFrequencyDeviation(float freqDev) override | nRF24 | virtual
setIrqAction(void(*func)(void)) | nRF24 |
setOutputPower(int8_t pwr) | nRF24 | virtual
setPacketReceivedAction(void(*func)(void)) | nRF24 | virtual
setPacketSentAction(void(*func)(void)) | nRF24 | virtual
setPreambleLength(size_t len) | PhysicalLayer | virtual
setReceivePipe(uint8_t pipeNum, uint8_t *addr) | nRF24 |
setReceivePipe(uint8_t pipeNum, uint8_t addrByte) | nRF24 |
setSyncWord(uint8_t *sync, size_t len) | PhysicalLayer | virtual
setTransmitPipe(uint8_t *addr) | nRF24 |
sleep() | nRF24 | virtual
standby() override | nRF24 | virtual
standby(uint8_t mode) override | nRF24 | virtual
startDirect() | PhysicalLayer |
startReceive() | nRF24 | virtual
startReceive(uint32_t timeout, uint16_t irqFlags, uint16_t irqMask, size_t len) | nRF24 | virtual
startTransmit(uint8_t *data, size_t len, uint8_t addr) override | nRF24 | virtual
startTransmit(const char *str, uint8_t addr=0) | nRF24 |
startTransmit(uint8_t *data, size_t len, uint8_t addr=0) | nRF24 |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmit(uint8_t *data, size_t len, uint8_t addr) override | nRF24 | virtual
transmit(const char *str, uint8_t addr=0) | nRF24 |
transmit(uint8_t *data, size_t len, uint8_t addr=0) | nRF24 |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | nRF24 | virtual