# RadioLib: src/modules/Si443x/Si4431.h Source File

Si4431.h
#if !defined(_RADIOLIB_SI4431_H)
#define _RADIOLIB_SI4431_H
#include "../../TypeDef.h"
#if !defined(RADIOLIB_EXCLUDE_SI443X)
#include "../../Module.h"
#include "Si4432.h"
class Si4431: public Si4432 {
public:
// constructor
Si4431(Module* mod);
// basic methods
int16_t begin(float freq = 434.0, float br = 4.8, float freqDev = 5.0, float rxBw = 181.1, int8_t power = 10, uint8_t preambleLen = 16);
// configuration methods
int16_t setOutputPower(int8_t power);
#if !defined(RADIOLIB_GODMODE)
protected:
#endif
#if !defined(RADIOLIB_GODMODE)
private:
#endif
};
#endif
#endif
Module
Implements all common low-level methods to control the wireless module. Every module class contains o...
Definition: Module.h:31
Si4431
Derived class for Si4431 modules.
Definition: Si4431.h:15
Si4431::Si4431
Si4431(Module *mod)
Default constructor.
Definition: Si4431.cpp:4
Si4431::begin
int16_t begin(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=181.1, int8_t power=10, uint8_t preambleLen=16)
Initialization method. Must be called at least once from Arduino sketch to initialize the module.
Definition: Si4431.cpp:8
Si4431::setOutputPower
int16_t setOutputPower(int8_t power)
Sets output power. Allowed values range from -8 to 13 dBm in 3 dBm steps.
Definition: Si4431.cpp:24
Si4432
Derived class for Si4432 modules.
Definition: Si4432.h:15