# RadioLib: Member List

SX1282 Member List

This is the complete list of members for SX1282, including all inherited members.

available() | PhysicalLayer |
begin(float freq=2400.0, float bw=812.5, uint8_t sf=9, uint8_t cr=7, uint8_t syncWord=RADIOLIB_SX128X_SYNC_WORD_PRIVATE, int8_t pwr=10, uint16_t preambleLength=12) | SX128x |
beginBLE(float freq=2400.0, uint16_t br=800, float freqDev=400.0, int8_t pwr=10, uint8_t dataShaping=RADIOLIB_SHAPING_0_5) | SX128x |
beginFLRC(float freq=2400.0, uint16_t br=650, uint8_t cr=3, int8_t pwr=10, uint16_t preambleLength=16, uint8_t dataShaping=RADIOLIB_SHAPING_0_5) | SX128x |
beginGFSK(float freq=2400.0, uint16_t br=800, float freqDev=400.0, int8_t pwr=10, uint16_t preambleLength=16) | SX128x |
calculateRxTimeout(RadioLibTime_t timeoutUs) | PhysicalLayer | virtual
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t pwr, int8_t *clipped) override | SX128x | virtual
clearChannelScanAction() | PhysicalLayer | virtual
clearDio1Action() | SX128x |
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqFlags(uint32_t irq) override | SX128x | virtual
clearPacketReceivedAction() override | SX128x | virtual
clearPacketSentAction() override | SX128x | virtual
dropSync() | PhysicalLayer |
explicitHeader() | SX128x |
finishTransmit() override | SX128x | virtual
getChannelScanResult() override | SX128x | virtual
getFreqStep() const | PhysicalLayer |
getFrequencyError() | SX128x |
getIrqFlags() override | SX128x | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getIrqStatus() | SX128x |
getPacketLength(bool update=true) override | SX128x | virtual
getPacketLength(bool update, uint8_t *offset) | SX128x |
getRangingResult() | SX1280 |
getRSSI() override | SX128x | virtual
getRSSI(bool packet) | SX128x |
getSNR() override | SX128x | virtual
getTimeOnAir(size_t len) override | SX128x | virtual
implicitHeader(size_t len) | SX128x |
invertIQ(bool enable) override | SX128x | virtual
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | SX128x | virtual
range(bool master, uint32_t addr, uint16_t calTable[3][6]=NULL) | SX1280 |
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | SX128x | virtual
readData(uint8_t *data, size_t len) override | SX128x | virtual
readData(uint8_t *data, size_t len) | SX128x |
receive(uint8_t *data, size_t len) override | SX128x | virtual
receive(uint8_t *data, size_t len) | SX128x |
receiveDirect() override | SX128x | virtual
reset(bool verify=true) | SX128x |
scanChannel() override | SX128x | virtual
scanChannel(const ChannelScanConfig_t &config) override | SX128x | virtual
setAccessAddress(uint32_t addr) | SX128x |
setBandwidth(float bw) | SX128x |
setBitRate(float br) override | SX128x | virtual
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setCodingRate(uint8_t cr, bool longInterleaving=false) | SX128x |
setCRC(uint8_t len, uint32_t initial=0x1D0F, uint16_t polynomial=0x1021) | SX128x |
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) override | SX128x | virtual
setDio1Action(void(*func)(void)) | SX128x |
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) override | SX128x | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | SX128x | virtual
setFrequency(float freq) override | SX128x | virtual
setFrequencyDeviation(float freqDev) override | SX128x | virtual
setGainControl(uint8_t gain=0) | SX128x |
setHighSensitivityMode(bool enable) | SX128x |
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqFlags(uint32_t irq) override | SX128x | virtual
setOutputPower(int8_t pwr) override | SX128x | virtual
setPacketReceivedAction(void(*func)(void)) override | SX128x | virtual
setPacketSentAction(void(*func)(void)) override | SX128x | virtual
setPreambleLength(uint32_t preambleLength) | SX128x |
PhysicalLayer::setPreambleLength(size_t len) | PhysicalLayer | virtual
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | SX128x |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | SX128x |
setSpreadingFactor(uint8_t sf) | SX128x |
setSyncWord(const uint8_t *syncWord, uint8_t len) | SX128x |
setSyncWord(uint8_t syncWord, uint8_t controlBits=0x44) | SX128x |
PhysicalLayer::setSyncWord(uint8_t *sync, size_t len) | PhysicalLayer | virtual
setWhitening(bool enabled) | SX128x |
sleep() override | SX128x | virtual
sleep(bool retainConfig) | SX128x |
standby() override | SX128x | virtual
standby(uint8_t mode, bool wakeup=false) | SX128x |
PhysicalLayer::standby(uint8_t mode) | PhysicalLayer | virtual
startChannelScan() override | SX128x | virtual
startChannelScan(const ChannelScanConfig_t &config) override | SX128x | virtual
startDirect() | PhysicalLayer |
startRanging(bool master, uint32_t addr, uint16_t calTable[3][6]=NULL) | SX1280 |
startReceive() override | SX128x | virtual
startReceive(uint16_t timeout, RadioLibIrqFlags_t irqFlags=RADIOLIB_IRQ_RX_DEFAULT_FLAGS, RadioLibIrqFlags_t irqMask=RADIOLIB_IRQ_RX_DEFAULT_MASK, size_t len=0) | SX128x |
PhysicalLayer::startReceive(uint32_t timeout, RadioLibIrqFlags_t irqFlags, RadioLibIrqFlags_t irqMask, size_t len) | PhysicalLayer | virtual
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX128x | virtual
startTransmit(const char *str, uint8_t addr=0) | SX128x |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX128x |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
SX1280(Module *mod) | SX1280 |
SX1281(Module *mod) | SX1281 |
SX1282(Module *mod) | SX1282 |
SX128x(Module *mod) | SX128x | explicit
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX128x | virtual
transmit(const char *str, uint8_t addr=0) | SX128x |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX128x |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | SX128x | virtual