# RadioLib: Member List

LoRaWANNode Member List

This is the complete list of members for LoRaWANNode, including all inherited members.

activateABP(uint8_t initialDr=RADIOLIB_LORAWAN_DATA_RATE_UNUSED) | LoRaWANNode |
activateOTAA(uint8_t initialDr=RADIOLIB_LORAWAN_DATA_RATE_UNUSED, LoRaWANJoinEvent_t *joinEvent=NULL) | LoRaWANNode | virtual
beginABP(uint32_t addr, uint8_t *fNwkSIntKey, uint8_t *sNwkSIntKey, uint8_t *nwkSEncKey, uint8_t *appSKey) | LoRaWANNode |
beginOTAA(uint64_t joinEUI, uint64_t devEUI, uint8_t *nwkKey, uint8_t *appKey) | LoRaWANNode |
clearSession() | LoRaWANNode |
dutyCycleInterval(RadioLibTime_t msPerHour, RadioLibTime_t airtime) | LoRaWANNode |
getAFCntDown() | LoRaWANNode |
getBufferNonces() | LoRaWANNode |
getBufferSession() | LoRaWANNode |
getDevAddr() | LoRaWANNode |
getFCntUp() | LoRaWANNode |
getLastToA() | LoRaWANNode |
getMacDeviceTimeAns(uint32_t *gpsEpoch, uint8_t *fraction, bool returnUnix=true) | LoRaWANNode |
getMacLinkCheckAns(uint8_t *margin, uint8_t *gwCnt) | LoRaWANNode |
getMaxPayloadLen() | LoRaWANNode |
getNFCntDown() | LoRaWANNode |
isActivated() | LoRaWANNode |
LoRaWANNode(PhysicalLayer *phy, const LoRaWANBand_t *band, uint8_t subBand=0) | LoRaWANNode |
resetFCntDown() | LoRaWANNode |
scanGuard | LoRaWANNode |
scheduleTransmission(RadioLibTime_t tUplink) | LoRaWANNode |
sendMacCommandReq(uint8_t cid) | LoRaWANNode |
sendReceive(const char *strUp, uint8_t fPort, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode | virtual
sendReceive(const char *strUp, uint8_t fPort, uint8_t *dataDown, size_t *lenDown, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode | virtual
sendReceive(uint8_t *dataUp, size_t lenUp, uint8_t fPort=1, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode | virtual
sendReceive(uint8_t *dataUp, size_t lenUp, uint8_t fPort, uint8_t *dataDown, size_t *lenDown, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode | virtual
setADR(bool enable=true) | LoRaWANNode |
setBufferNonces(uint8_t *persistentBuffer) | LoRaWANNode |
setBufferSession(uint8_t *persistentBuffer) | LoRaWANNode |
setCSMA(bool csmaEnabled, uint8_t maxChanges=4, uint8_t backoffMax=0, uint8_t difsSlots=2) | LoRaWANNode |
setDatarate(uint8_t drUp) | LoRaWANNode |
setDeviceStatus(uint8_t battLevel) | LoRaWANNode |
setDutyCycle(bool enable=true, RadioLibTime_t msPerHour=0) | LoRaWANNode |
setDwellTime(bool enable, RadioLibTime_t msPerUplink=0) | LoRaWANNode |
setRx2Dr(uint8_t dr) | LoRaWANNode |
setTxPower(int8_t txPower) | LoRaWANNode |
timeUntilUplink() | LoRaWANNode |
TS009 | LoRaWANNode |