# RadioLib: Member List

SX126x Member List

This is the complete list of members for SX126x, including all inherited members.

autoLDRO() | SX126x |
available() | PhysicalLayer |
begin(uint8_t cr, uint8_t syncWord, uint16_t preambleLength, float tcxoVoltage, bool useRegulatorLDO=false) | SX126x |
beginFSK(float br, float freqDev, float rxBw, uint16_t preambleLength, float tcxoVoltage, bool useRegulatorLDO=false) | SX126x |
calculateRxTimeout(RadioLibTime_t timeoutUs) override | SX126x | virtual
calibrateImageRejection(float freqMin, float freqMax) | SX126x |
checkDataRate(DataRate_t dr) override | SX126x | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) | PhysicalLayer | virtual
clearChannelScanAction() override | SX126x | virtual
clearDio1Action() | SX126x |
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqFlags(uint32_t irq) override | SX126x | virtual
clearPacketReceivedAction() override | SX126x | virtual
clearPacketSentAction() override | SX126x | virtual
disableAddressFiltering() | SX126x |
dropSync() | PhysicalLayer |
explicitHeader() | SX126x |
finishTransmit() override | SX126x | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_SX126X_MAX_PACKET_LENGTH) | SX126x |
forceLDRO(bool enable) | SX126x |
getChannelScanResult() override | SX126x | virtual
getCurrentLimit() | SX126x |
getDataRate() const | SX126x |
getFreqStep() const | PhysicalLayer |
getFrequencyError() | SX126x |
getIrqFlags() override | SX126x | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getPacketLength(bool update=true) override | SX126x | virtual
getPacketLength(bool update, uint8_t *offset) | SX126x |
getRSSI() override | SX126x | virtual
getRSSI(bool packet) | SX126x |
getSNR() override | SX126x | virtual
getTimeOnAir(size_t len) override | SX126x | virtual
implicitHeader(size_t len) | SX126x |
invertIQ(bool enable) override | SX126x | virtual
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | SX126x | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | SX126x | virtual
readData(uint8_t *data, size_t len) override | SX126x | virtual
readData(uint8_t *data, size_t len) | SX126x |
receive(uint8_t *data, size_t len) override | SX126x | virtual
receive(uint8_t *data, size_t len) | SX126x |
receiveDirect() override | SX126x | virtual
reset(bool verify=true) | SX126x |
scanChannel() override | SX126x | virtual
scanChannel(const ChannelScanConfig_t &config) override | SX126x | virtual
setBandwidth(float bw) | SX126x |
setBitRate(float br) override | SX126x | virtual
setBroadcastAddress(uint8_t broadAddr) | SX126x |
setChannelScanAction(void(*func)(void)) override | SX126x | virtual
setCodingRate(uint8_t cr) | SX126x |
setCRC(uint8_t len, uint16_t initial=0x1D0F, uint16_t polynomial=0x1021, bool inverted=true) | SX126x |
setCurrentLimit(float currentLimit) | SX126x |
setDataRate(DataRate_t dr) override | SX126x | virtual
setDataShaping(uint8_t sh) override | SX126x | virtual
setDio1Action(void(*func)(void)) | SX126x |
setDio2AsRfSwitch(bool enable=true) | SX126x |
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) override | SX126x | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | SX126x | virtual
setFrequency(float freq) | PhysicalLayer | virtual
setFrequencyDeviation(float freqDev) override | SX126x | virtual
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqFlags(uint32_t irq) override | SX126x | virtual
setNodeAddress(uint8_t nodeAddr) | SX126x |
setOutputPower(int8_t power) | PhysicalLayer | virtual
setPacketReceivedAction(void(*func)(void)) override | SX126x | virtual
setPacketSentAction(void(*func)(void)) override | SX126x | virtual
setPaConfig(uint8_t paDutyCycle, uint8_t deviceSel, uint8_t hpMax=RADIOLIB_SX126X_PA_CONFIG_HP_MAX, uint8_t paLut=RADIOLIB_SX126X_PA_CONFIG_PA_LUT) | SX126x |
setPaRampTime(uint8_t rampTime) | SX126x |
setPreambleLength(size_t preambleLength) override | SX126x | virtual
setRegulatorDCDC() | SX126x |
setRegulatorLDO() | SX126x |
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | SX126x |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | SX126x |
setRxBandwidth(float rxBw) | SX126x |
setRxBoostedGainMode(bool rxbgm, bool persist=true) | SX126x |
setSpreadingFactor(uint8_t sf) | SX126x |
setSyncBits(uint8_t *syncWord, uint8_t bitsLen) | SX126x |
setSyncWord(uint8_t syncWord, uint8_t controlBits=0x44) | SX126x |
setSyncWord(uint8_t *syncWord, size_t len) override | SX126x | virtual
setTCXO(float voltage, uint32_t delay=5000) | SX126x |
setWhitening(bool enabled, uint16_t initial=0x01FF) | SX126x |
sleep() override | SX126x | virtual
sleep(bool retainConfig) | SX126x |
spectralScanAbort() | SX126x |
spectralScanGetResult(uint16_t *results) | SX126x |
spectralScanGetStatus() | SX126x |
spectralScanStart(uint16_t numSamples, uint8_t window=RADIOLIB_SX126X_SPECTRAL_SCAN_WINDOW_DEFAULT, uint8_t interval=RADIOLIB_SX126X_SCAN_INTERVAL_8_20_US) | SX126x |
standby() override | SX126x | virtual
standby(uint8_t mode, bool wakeup=true) | SX126x |
PhysicalLayer::standby(uint8_t mode) | PhysicalLayer | virtual
standbyXOSC | SX126x |
startChannelScan() override | SX126x | virtual
startChannelScan(const ChannelScanConfig_t &config) override | SX126x | virtual
startDirect() | PhysicalLayer |
startReceive() override | SX126x | virtual
startReceive(uint32_t timeout, RadioLibIrqFlags_t irqFlags=RADIOLIB_IRQ_RX_DEFAULT_FLAGS, RadioLibIrqFlags_t irqMask=RADIOLIB_IRQ_RX_DEFAULT_MASK, size_t len=0) | SX126x | virtual
startReceiveDutyCycle(uint32_t rxPeriod, uint32_t sleepPeriod, RadioLibIrqFlags_t irqFlags=RADIOLIB_IRQ_RX_DEFAULT_FLAGS, RadioLibIrqFlags_t irqMask=RADIOLIB_IRQ_RX_DEFAULT_MASK) | SX126x |
startReceiveDutyCycleAuto(uint16_t senderPreambleLength=0, uint16_t minSymbols=8, RadioLibIrqFlags_t irqFlags=RADIOLIB_IRQ_RX_DEFAULT_FLAGS, RadioLibIrqFlags_t irqMask=RADIOLIB_IRQ_RX_DEFAULT_MASK) | SX126x |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX126x | virtual
startTransmit(const char *str, uint8_t addr=0) | SX126x |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX126x |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
SX126x(Module *mod) | SX126x | explicit
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX126x | virtual
transmit(const char *str, uint8_t addr=0) | SX126x |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX126x |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | SX126x | virtual
uploadPatch(const uint32_t *patch, size_t len, bool nonvolatile=true) | SX126x |
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_SX126X_MAX_PACKET_LENGTH) | SX126x |
XTAL | SX126x |