# RadioLib: Member List

PhysicalLayer Member List

This is the complete list of members for PhysicalLayer, including all inherited members.

AFSKClient (defined in PhysicalLayer) | PhysicalLayer | friend
available() | PhysicalLayer |
AX25Client (defined in PhysicalLayer) | PhysicalLayer | friend
BellClient (defined in PhysicalLayer) | PhysicalLayer | friend
calculateRxTimeout(RadioLibTime_t timeoutUs) | PhysicalLayer | virtual
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) | PhysicalLayer | virtual
clearChannelScanAction() | PhysicalLayer | virtual
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqFlags(uint32_t irq) | PhysicalLayer | virtual
clearPacketReceivedAction() | PhysicalLayer | virtual
clearPacketSentAction() | PhysicalLayer | virtual
dropSync() | PhysicalLayer |
finishTransmit() | PhysicalLayer | virtual
FSK4Client (defined in PhysicalLayer) | PhysicalLayer | friend
FT8Client (defined in PhysicalLayer) | PhysicalLayer | friend
getChannelScanResult() | PhysicalLayer | virtual
getFreqStep() const | PhysicalLayer |
getIrqFlags() | PhysicalLayer | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getPacketLength(bool update=true) | PhysicalLayer | virtual
getRSSI() | PhysicalLayer | virtual
getSNR() | PhysicalLayer | virtual
getTimeOnAir(size_t len) | PhysicalLayer | virtual
HellClient (defined in PhysicalLayer) | PhysicalLayer | friend
invertIQ(bool enable) | PhysicalLayer | virtual
LoRaWANNode (defined in PhysicalLayer) | PhysicalLayer | friend
MorseClient (defined in PhysicalLayer) | PhysicalLayer | friend
PagerClient (defined in PhysicalLayer) | PhysicalLayer | friend
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() | PhysicalLayer | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) | PhysicalLayer | virtual
readData(uint8_t *data, size_t len) | PhysicalLayer | virtual
receive(uint8_t *data, size_t len) | PhysicalLayer | virtual
receiveDirect() | PhysicalLayer | virtual
RTTYClient (defined in PhysicalLayer) | PhysicalLayer | friend
scanChannel() | PhysicalLayer | virtual
scanChannel(const ChannelScanConfig_t &config) | PhysicalLayer | virtual
setBitRate(float br) | PhysicalLayer | virtual
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) | PhysicalLayer | virtual
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) | PhysicalLayer | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) | PhysicalLayer | virtual
setFrequency(float freq) | PhysicalLayer | virtual
setFrequencyDeviation(float freqDev) | PhysicalLayer | virtual
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqFlags(uint32_t irq) | PhysicalLayer | virtual
setOutputPower(int8_t power) | PhysicalLayer | virtual
setPacketReceivedAction(void(*func)(void)) | PhysicalLayer | virtual
setPacketSentAction(void(*func)(void)) | PhysicalLayer | virtual
setPreambleLength(size_t len) | PhysicalLayer | virtual
setSyncWord(uint8_t *sync, size_t len) | PhysicalLayer | virtual
sleep() | PhysicalLayer | virtual
SSTVClient (defined in PhysicalLayer) | PhysicalLayer | friend
standby() | PhysicalLayer | virtual
standby(uint8_t mode) | PhysicalLayer | virtual
startChannelScan() | PhysicalLayer | virtual
startChannelScan(const ChannelScanConfig_t &config) | PhysicalLayer | virtual
startDirect() | PhysicalLayer |
startReceive() | PhysicalLayer | virtual
startReceive(uint32_t timeout, RadioLibIrqFlags_t irqFlags, RadioLibIrqFlags_t irqMask, size_t len) | PhysicalLayer | virtual
startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | PhysicalLayer | virtual
transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | PhysicalLayer | virtual
transmitDirect(uint32_t frf=0) | PhysicalLayer | virtual