# RadioLib: src/BuildOpt.h Source File

BuildOpt.h
#if !defined(_RADIOLIB_BUILD_OPTIONS_H)
#define _RADIOLIB_BUILD_OPTIONS_H
#include "TypeDef.h"
/* RadioLib build configuration options */
/*
* Debug output enable.
* Warning: Debug output will slow down the whole system significantly.
* Also, it will result in larger compiled binary.
* Levels: basic - only main info
* protocol - mainly LoRaWAN stuff, but other protocols as well
* SPI - full transcript of all SPI communication
*/
#if !defined(RADIOLIB_DEBUG_BASIC)
#define RADIOLIB_DEBUG_BASIC (0)
#endif
#if !defined(RADIOLIB_DEBUG_PROTOCOL)
#define RADIOLIB_DEBUG_PROTOCOL (0)
#endif
#if !defined(RADIOLIB_DEBUG_SPI)
#define RADIOLIB_DEBUG_SPI (0)
#endif
#if !defined(RADIOLIB_VERBOSE_ASSERT)
#define RADIOLIB_VERBOSE_ASSERT (0)
#endif
// set which output port should be used for debug output
// may be Serial port (on Arduino) or file like stdout or stderr (on generic platforms)
#if !defined(RADIOLIB_DEBUG_PORT)
#define RADIOLIB_DEBUG_PORT Serial
#endif
/*
* Comment to disable "paranoid" SPI mode, or set RADIOLIB_SPI_PARANOID to 0
* Every write to an SPI register using SPI set function will be verified by a subsequent read operation.
* This improves reliability, but slightly slows down communication.
* Note: Enabled by default.
*/
#if !defined(RADIOLIB_SPI_PARANOID)
#define RADIOLIB_SPI_PARANOID (1)
#endif
/*
* Comment to disable parameter range checking
* RadioLib will check provided parameters (such as frequency) against limits determined by the device manufacturer.
* It is highly advised to keep this macro defined, removing it will allow invalid values to be set,
* possibly leading to bricked module and/or program crashing.
* Note: Enabled by default.
*/
#if !defined(RADIOLIB_CHECK_PARAMS)
#define RADIOLIB_CHECK_PARAMS (1)
#endif
/*
* SX127x errata fix enable
* Warning: SX127x errata fix has been reported to cause issues with LoRa bandwidths lower than 62.5 kHz.
* It should only be enabled if you really are observing some errata-related issue.
* Note: Disabled by default.
*/
#if !defined(RADIOLIB_FIX_ERRATA_SX127X)
#define RADIOLIB_FIX_ERRATA_SX127X (0)
#endif
/*
* God mode enable - all methods and member variables in all classes will be made public, thus making them accessible from Arduino code.
* Warning: Come on, it's called GOD mode - obviously only use this if you know what you're doing.
* Failure to heed the above warning may result in bricked module.
*/
#if !defined(RADIOLIB_GODMODE)
#define RADIOLIB_GODMODE (0)
#endif
/*
* Low-level hardware access enable
* This will make some hardware methods like SPI get/set accessible from the user sketch - think of it as "god mode lite"
* Warning: RadioLib won't stop you from writing invalid stuff into your device, so it's quite easy to brick your module with this.
*/
#if !defined(RADIOLIB_LOW_LEVEL)
#define RADIOLIB_LOW_LEVEL (0)
#endif
/*
* Enable pre-defined modules when using RadioShield, disabled by default.
*/
#if !defined(RADIOLIB_RADIOSHIELD)
#define RADIOLIB_RADIOSHIELD (0)
#endif
/*
* Enable interrupt-based timing control
* For details, see https://github.com/jgromes/RadioLib/wiki/Interrupt-Based-Timing
*/
#if !defined(RADIOLIB_INTERRUPT_TIMING)
#define RADIOLIB_INTERRUPT_TIMING (0)
#endif
/*
* Enable static-only memory management: no dynamic allocation will be performed.
* Warning: Large static arrays will be created in some methods. It is not advised to send large packets in this mode.
*/
#if !defined(RADIOLIB_STATIC_ONLY)
#define RADIOLIB_STATIC_ONLY (0)
#endif
// set the size of static arrays to use
#if !defined(RADIOLIB_STATIC_ARRAY_SIZE)
#define RADIOLIB_STATIC_ARRAY_SIZE (256)
#endif
/*
* Uncomment on boards whose clock runs too slow or too fast
* Set the value according to the following scheme:
* Enable timestamps on your terminal
* Print something to terminal, wait 1000 milliseconds, print something again
* If the difference is e.g. 1014 milliseconds between the prints, set this value to 14
* Or, for more accuracy, wait for 100,000 milliseconds and divide the total drift by 100
*/
#if !defined(RADIOLIB_CLOCK_DRIFT_MS)
//#define RADIOLIB_CLOCK_DRIFT_MS (0)
#endif
#if ARDUINO >= 100
// Arduino build
#include "Arduino.h"
#define RADIOLIB_BUILD_ARDUINO
#else
// generic build
#include <stdio.h>
#define RADIOLIB_BUILD_GENERIC
#endif
#if defined(RADIOLIB_BUILD_ARDUINO)
/*
* Platform-specific configuration.
*
* RADIOLIB_PLATFORM - platform name, used in debugging to quickly check the correct platform is detected.
* RADIOLIB_NC - alias for unused pin, usually the largest possible value of uint8_t.
* RADIOLIB_DEFAULT_SPI - default SPIClass instance to use.
* RADIOLIB_NONVOLATILE - macro to place variable into program storage (usually Flash).
* RADIOLIB_NONVOLATILE_READ_BYTE - function/macro to read variables saved in program storage (usually Flash).
* RADIOLIB_TYPE_ALIAS - construct to create an alias for a type, usually vai the `using` keyword.
* RADIOLIB_TONE_UNSUPPORTED - some platforms do not have tone()/noTone(), which is required for AFSK.
* RADIOLIB_BUILTIN_MODULE - some platforms have a builtin radio module on fixed pins, this macro is used to specify that pinout.
*
* In addition, some platforms may require RadioLib to disable specific drivers (such as ESP8266).
*
* Users may also specify their own configuration by uncommenting the RADIOLIB_CUSTOM_ARDUINO,
* and then specifying all platform parameters in the section below. This will override automatic
* platform detection.
*/
// uncomment to enable custom platform definition
//#define RADIOLIB_CUSTOM_ARDUINO
#if defined(RADIOLIB_CUSTOM_ARDUINO)
// name for your platform
#define RADIOLIB_PLATFORM "Custom"
// the following must be defined if the Arduino core does not support tone or yield function
//#define RADIOLIB_TONE_UNSUPPORTED
//#define RADIOLIB_YIELD_UNSUPPORTED
// in addition, the following macros may be defined if the Arduino core differs from the defaults
#define RADIOLIB_NC (0xFFFFFFFF)
#define RADIOLIB_DEFAULT_SPI SPI
#define RADIOLIB_DEFAULT_SPI_SETTINGS SPISettings(2000000, MSBFIRST, SPI_MODE0)
#define RADIOLIB_NONVOLATILE PROGMEM
#define RADIOLIB_NONVOLATILE_READ_BYTE(addr) pgm_read_byte(addr)
#define RADIOLIB_NONVOLATILE_READ_DWORD(addr) pgm_read_dword(addr)
#define RADIOLIB_TYPE_ALIAS(type, alias) using alias = type;
// you might also have to define these if the Arduino core has some uncommon pin mode/status types
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST
// some of RadioLib drivers may be excluded, to prevent collisions with platforms (or to speed up build process)
// the following is a complete list of all possible exclusion macros, uncomment any of them to disable that driver
// NOTE: Some of the exclusion macros are dependent on each other. For example, it is not possible to exclude RF69
// while keeping SX1231 (because RF69 is the base class for SX1231). The dependency is always uni-directional,
// so excluding SX1231 and keeping RF69 is valid.
//#define RADIOLIB_EXCLUDE_CC1101 (1)
//#define RADIOLIB_EXCLUDE_NRF24 (1)
//#define RADIOLIB_EXCLUDE_RF69 (1)
//#define RADIOLIB_EXCLUDE_SX1231 (1) // dependent on RADIOLIB_EXCLUDE_RF69
//#define RADIOLIB_EXCLUDE_SI443X (1)
//#define RADIOLIB_EXCLUDE_RFM2X (1) // dependent on RADIOLIB_EXCLUDE_SI443X
//#define RADIOLIB_EXCLUDE_SX127X (1)
//#define RADIOLIB_EXCLUDE_SX126X (1)
//#define RADIOLIB_EXCLUDE_STM32WLX (1) // dependent on RADIOLIB_EXCLUDE_SX126X
//#define RADIOLIB_EXCLUDE_SX128X (1)
//#define RADIOLIB_EXCLUDE_AFSK (1)
//#define RADIOLIB_EXCLUDE_AX25 (1)
//#define RADIOLIB_EXCLUDE_HELLSCHREIBER (1)
//#define RADIOLIB_EXCLUDE_MORSE (1)
//#define RADIOLIB_EXCLUDE_RTTY (1)
//#define RADIOLIB_EXCLUDE_SSTV (1)
//#define RADIOLIB_EXCLUDE_DIRECT_RECEIVE (1)
#elif defined(__AVR__) && !(defined(ARDUINO_AVR_UNO_WIFI_REV2) || defined(ARDUINO_AVR_NANO_EVERY) || defined(ARDUINO_ARCH_MEGAAVR))
// Arduino AVR boards (except for megaAVR) - Uno, Mega etc.
#define RADIOLIB_PLATFORM "Arduino AVR"
#if !(defined(__AVR_ATmega1280__) || defined(__AVR_ATmega2560__) || defined(__AVR_ATmega1284__) || defined(__AVR_ATmega1284P__))
#define RADIOLIB_LOWEND_PLATFORM
#endif
#elif defined(ESP8266)
// ESP8266 boards
#define RADIOLIB_PLATFORM "ESP8266"
#elif defined(ESP32) || defined(ARDUINO_ARCH_ESP32)
#define RADIOLIB_ESP32
// ESP32 boards
#define RADIOLIB_PLATFORM "ESP32"
// ESP32 doesn't support tone(), but it can be emulated via LED control peripheral
#define RADIOLIB_TONE_UNSUPPORTED
#define RADIOLIB_TONE_ESP32_CHANNEL (1)
#elif defined(ARDUINO_ARCH_STM32)
// official STM32 Arduino core (https://github.com/stm32duino/Arduino_Core_STM32)
#define RADIOLIB_PLATFORM "Arduino STM32 (official)"
#elif defined(SAMD_SERIES)
// Adafruit SAMD boards (M0 and M4)
#define RADIOLIB_PLATFORM "Adafruit SAMD"
#elif defined(ARDUINO_ARCH_SAMD)
// Arduino SAMD (Zero, MKR, etc.)
#define RADIOLIB_PLATFORM "Arduino SAMD"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
#elif defined(__SAM3X8E__)
// Arduino Due
#define RADIOLIB_PLATFORM "Arduino Due"
#define RADIOLIB_TONE_UNSUPPORTED
#elif (defined(NRF52832_XXAA) || defined(NRF52840_XXAA)) && !defined(ARDUINO_ARDUINO_NANO33BLE)
// Adafruit nRF52 boards
#define RADIOLIB_PLATFORM "Adafruit nRF52"
#elif defined(ARDUINO_ARC32_TOOLS)
// Intel Curie
#define RADIOLIB_PLATFORM "Intel Curie"
#elif defined(ARDUINO_AVR_UNO_WIFI_REV2) || defined(ARDUINO_AVR_NANO_EVERY) || defined(PORTDUINO)
// Arduino megaAVR boards - Uno Wifi Rev.2, Nano Every
#define RADIOLIB_PLATFORM "Arduino megaAVR"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
#elif defined(ARDUINO_ARCH_APOLLO3)
// Sparkfun Apollo3 boards
#define RADIOLIB_PLATFORM "Sparkfun Apollo3"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (Arduino_PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
#elif defined(ARDUINO_ARDUINO_NANO33BLE)
// Arduino Nano 33 BLE
#define RADIOLIB_PLATFORM "Arduino Nano 33 BLE"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
// Arduino mbed OS boards have a really bad tone implementation which will crash after a couple seconds
#define RADIOLIB_TONE_UNSUPPORTED
#define RADIOLIB_MBED_TONE_OVERRIDE
#elif defined(ARDUINO_PORTENTA_H7_M7) || defined(ARDUINO_PORTENTA_H7_M4)
// Arduino Portenta H7
#define RADIOLIB_PLATFORM "Portenta H7"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
// Arduino mbed OS boards have a really bad tone implementation which will crash after a couple seconds
#define RADIOLIB_TONE_UNSUPPORTED
#define RADIOLIB_MBED_TONE_OVERRIDE
#elif defined(__STM32F4__) || defined(__STM32F1__)
// Arduino STM32 core by Roger Clark (https://github.com/rogerclarkmelbourne/Arduino_STM32)
#define RADIOLIB_PLATFORM "STM32duino (unofficial)"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (WiringPinMode)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (ExtIntTriggerMode)
#elif defined(ARDUINO_ARCH_MEGAAVR)
// MegaCoreX by MCUdude (https://github.com/MCUdude/MegaCoreX)
#define RADIOLIB_PLATFORM "MegaCoreX"
#elif defined(ARDUINO_ARCH_MBED_RP2040)
// Raspberry Pi Pico (official mbed core)
#define RADIOLIB_PLATFORM "Raspberry Pi Pico"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
// Arduino mbed OS boards have a really bad tone implementation which will crash after a couple seconds
#define RADIOLIB_TONE_UNSUPPORTED
#define RADIOLIB_MBED_TONE_OVERRIDE
#elif defined(ARDUINO_ARCH_RP2040)
// Raspberry Pi Pico (unofficial core)
#define RADIOLIB_PLATFORM "Raspberry Pi Pico (unofficial)"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
#elif defined(__ASR6501__) || defined(ARDUINO_ARCH_ASR650X) || defined(DARDUINO_ARCH_ASR6601)
// CubeCell
#define RADIOLIB_PLATFORM "CubeCell"
#define RADIOLIB_DEFAULT_SPI_SETTINGS SPISettings(1000000, MSBFIRST, SPI_MODE0) // see issue #709
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PINMODE)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (IrqModes)
// provide an easy access to the on-board module
#include "board-config.h"
#define RADIOLIB_BUILTIN_MODULE RADIO_NSS, RADIO_DIO_1, RADIO_RESET, RADIO_BUSY
// CubeCell doesn't seem to define nullptr, let's do something like that now
#define nullptr NULL
// ... and also defines pinMode() as a macro, which is by far the stupidest thing I have seen on Arduino
#undef pinMode
// ... and uses an outdated GCC which does not support type aliases
#define RADIOLIB_TYPE_ALIAS(type, alias) typedef class type alias;
// ... and it also has no tone(). This platform was designed by an idiot.
#define RADIOLIB_TONE_UNSUPPORTED
// ... AND as the (hopefully) final nail in the coffin, IT F*CKING DEFINES YIELD() AS A MACRO THAT DOES NOTHING!!!
#define RADIOLIB_YIELD_UNSUPPORTED
#if defined(yield)
#undef yield
#endif
#elif defined(RASPI)
// RaspiDuino framework (https://github.com/me-no-dev/RasPiArduino)
#define RADIOLIB_PLATFORM "RasPiArduino"
// let's start off easy - no tone on this platform, that can happen
#define RADIOLIB_TONE_UNSUPPORTED
// hmm, no yield either - weird on something like Raspberry PI, but sure, we can handle it
#define RADIOLIB_YIELD_UNSUPPORTED
// aight, getting to the juicy stuff - PGM_P seems missing, that's the first time
#define PGM_P const char *
// ... and for the grand finale, we have millis() and micros() DEFINED AS MACROS!
#if defined(millis)
#undef millis
inline RadioLibTime_t millis() { return((RadioLibTime_t)(STCV / 1000)); };
#endif
#if defined(micros)
#undef micros
inline RadioLibTime_t micros() { return((RadioLibTime_t)(STCV)); };
#endif
#elif defined(TEENSYDUINO)
// Teensy
#define RADIOLIB_PLATFORM "Teensy"
#elif defined(ARDUINO_ARCH_RENESAS)
// Arduino Renesas (UNO R4)
#define RADIOLIB_PLATFORM "Arduino Renesas (UNO R4)"
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST (PinMode)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST (PinStatus)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST (PinStatus)
#else
// other Arduino platforms not covered by the above list - this may or may not work
#define RADIOLIB_PLATFORM "Unknown Arduino"
#define RADIOLIB_UNKNOWN_PLATFORM
#endif
// set the default values for all macros
// these will be applied if they were not defined above
#if !defined(RADIOLIB_NC)
#define RADIOLIB_NC (0xFFFFFFFF)
#endif
#if !defined(RADIOLIB_DEFAULT_SPI)
#define RADIOLIB_DEFAULT_SPI SPI
#endif
#if !defined(RADIOLIB_DEFAULT_SPI_SETTINGS)
#define RADIOLIB_DEFAULT_SPI_SETTINGS SPISettings(2000000, MSBFIRST, SPI_MODE0)
#endif
#if !defined(RADIOLIB_NONVOLATILE)
#define RADIOLIB_NONVOLATILE PROGMEM
#endif
#if !defined(RADIOLIB_NONVOLATILE_PTR)
#define RADIOLIB_NONVOLATILE_PTR PGM_P
#endif
#if !defined(RADIOLIB_NONVOLATILE_READ_BYTE)
#define RADIOLIB_NONVOLATILE_READ_BYTE(addr) pgm_read_byte(addr)
#endif
#if !defined(RADIOLIB_NONVOLATILE_READ_DWORD)
#define RADIOLIB_NONVOLATILE_READ_DWORD(addr) pgm_read_dword(addr)
#endif
#if !defined(RADIOLIB_TYPE_ALIAS)
#define RADIOLIB_TYPE_ALIAS(type, alias) using alias = type;
#endif
#if !defined(RADIOLIB_ARDUINOHAL_PIN_MODE_CAST)
#define RADIOLIB_ARDUINOHAL_PIN_MODE_CAST
#endif
#if !defined(RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST)
#define RADIOLIB_ARDUINOHAL_PIN_STATUS_CAST
#endif
#if !defined(RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST)
#define RADIOLIB_ARDUINOHAL_INTERRUPT_MODE_CAST
#endif
#else
// generic non-Arduino platform
#define RADIOLIB_PLATFORM "Generic"
#define RADIOLIB_NC (0xFF)
#define RADIOLIB_NONVOLATILE
#define RADIOLIB_NONVOLATILE_READ_BYTE(addr) (*((uint8_t *)(void *)(addr)))
#define RADIOLIB_NONVOLATILE_READ_DWORD(addr) (*((uint32_t *)(void *)(addr)))
#define RADIOLIB_TYPE_ALIAS(type, alias) using alias = type;
#if !defined(RADIOLIB_DEBUG_PORT)
#define RADIOLIB_DEBUG_PORT stdout
#endif
#define DEC 10
#define HEX 16
#define OCT 8
#define BIN 2
#include <stdint.h>
#endif
// This only compiles on STM32 boards with SUBGHZ module, but also
// include when generating docs
#if (!defined(ARDUINO_ARCH_STM32) || !defined(SUBGHZSPI_BASE)) && !defined(DOXYGEN)
#define RADIOLIB_EXCLUDE_STM32WLX (1)
#endif
// if verbose assert is enabled, enable basic debug too
#if RADIOLIB_VERBOSE_ASSERT
#define RADIOLIB_DEBUG (1)
#endif
// set the global debug mode flag
#if RADIOLIB_DEBUG_BASIC || RADIOLIB_DEBUG_PROTOCOL || RADIOLIB_DEBUG_SPI
#define RADIOLIB_DEBUG (1)
#else
#define RADIOLIB_DEBUG (0)
#endif
#if RADIOLIB_DEBUG
#if defined(RADIOLIB_BUILD_ARDUINO)
#define RADIOLIB_DEBUG_PRINT(...) Module::serialPrintf(__VA_ARGS__)
#define RADIOLIB_DEBUG_PRINTLN(M, ...) Module::serialPrintf(M "\n", ##__VA_ARGS__)
#define RADIOLIB_DEBUG_PRINT_LVL(LEVEL, M, ...) Module::serialPrintf(LEVEL "" M, ##__VA_ARGS__)
#define RADIOLIB_DEBUG_PRINTLN_LVL(LEVEL, M, ...) Module::serialPrintf(LEVEL "" M "\n", ##__VA_ARGS__)
// some platforms do not support printf("%f"), so it has to be done this way
#define RADIOLIB_DEBUG_PRINT_FLOAT(LEVEL, VAL, DECIMALS) RADIOLIB_DEBUG_PRINT(LEVEL); RADIOLIB_DEBUG_PORT.print(VAL, DECIMALS)
#else
#if !defined(RADIOLIB_DEBUG_PRINT)
#define RADIOLIB_DEBUG_PRINT(...) fprintf(RADIOLIB_DEBUG_PORT, __VA_ARGS__)
#define RADIOLIB_DEBUG_PRINT_LVL(LEVEL, M, ...) fprintf(RADIOLIB_DEBUG_PORT, LEVEL "" M, ##__VA_ARGS__)
#endif
#if !defined(RADIOLIB_DEBUG_PRINTLN)
#define RADIOLIB_DEBUG_PRINTLN(M, ...) fprintf(RADIOLIB_DEBUG_PORT, M "\n", ##__VA_ARGS__)
#define RADIOLIB_DEBUG_PRINTLN_LVL(LEVEL, M, ...) fprintf(RADIOLIB_DEBUG_PORT, LEVEL "" M "\n", ##__VA_ARGS__)
#endif
#define RADIOLIB_DEBUG_PRINT_FLOAT(LEVEL, VAL, DECIMALS) RADIOLIB_DEBUG_PRINT(LEVEL "%.3f", VAL)
#endif
#define RADIOLIB_DEBUG_HEXDUMP(LEVEL, ...) Module::hexdump(LEVEL, __VA_ARGS__)
#else
#define RADIOLIB_DEBUG_PRINT(...) {}
#define RADIOLIB_DEBUG_PRINTLN(...) {}
#define RADIOLIB_DEBUG_PRINT_FLOAT(VAL, DECIMALS) {}
#define RADIOLIB_DEBUG_HEXDUMP(...) {}
#endif
#if RADIOLIB_DEBUG_BASIC
#define RADIOLIB_DEBUG_BASIC_PRINT(...) RADIOLIB_DEBUG_PRINT_LVL("RLB_DBG: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_BASIC_PRINT_NOTAG(...) RADIOLIB_DEBUG_PRINT_LVL("", __VA_ARGS__)
#define RADIOLIB_DEBUG_BASIC_PRINTLN(...) RADIOLIB_DEBUG_PRINTLN_LVL("RLB_DBG: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_BASIC_PRINT_FLOAT(...) RADIOLIB_DEBUG_PRINT_FLOAT("RLB_DBG: ", __VA_ARGS__);
#define RADIOLIB_DEBUG_BASIC_HEXDUMP(...) RADIOLIB_DEBUG_HEXDUMP("RLB_DBG: ", __VA_ARGS__);
#else
#define RADIOLIB_DEBUG_BASIC_PRINT(...) {}
#define RADIOLIB_DEBUG_BASIC_PRINT_NOTAG(...) {}
#define RADIOLIB_DEBUG_BASIC_PRINTLN(...) {}
#define RADIOLIB_DEBUG_BASIC_PRINT_FLOAT(...) {}
#define RADIOLIB_DEBUG_BASIC_HEXDUMP(...) {}
#endif
#if RADIOLIB_DEBUG_PROTOCOL
#define RADIOLIB_DEBUG_PROTOCOL_PRINT(...) RADIOLIB_DEBUG_PRINT_LVL("RLB_PRO: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_PROTOCOL_PRINTLN(...) RADIOLIB_DEBUG_PRINTLN_LVL("RLB_PRO: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_PROTOCOL_PRINT_FLOAT(...) RADIOLIB_DEBUG_PRINT_FLOAT("RLB_PRO: ", __VA_ARGS__);
#define RADIOLIB_DEBUG_PROTOCOL_HEXDUMP(...) RADIOLIB_DEBUG_HEXDUMP("RLB_PRO: ", __VA_ARGS__);
#else
#define RADIOLIB_DEBUG_PROTOCOL_PRINT(...) {}
#define RADIOLIB_DEBUG_PROTOCOL_PRINTLN(...) {}
#define RADIOLIB_DEBUG_PROTOCOL_PRINT_FLOAT(...) {}
#define RADIOLIB_DEBUG_PROTOCOL_HEXDUMP(...) {}
#endif
#if RADIOLIB_DEBUG_SPI
#define RADIOLIB_DEBUG_SPI_PRINT(...) RADIOLIB_DEBUG_PRINT_LVL("RLB_SPI: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_SPI_PRINT_NOTAG(...) RADIOLIB_DEBUG_PRINT_LVL("", __VA_ARGS__)
#define RADIOLIB_DEBUG_SPI_PRINTLN(...) RADIOLIB_DEBUG_PRINTLN_LVL("RLB_SPI: ", __VA_ARGS__)
#define RADIOLIB_DEBUG_SPI_PRINTLN_NOTAG(...) RADIOLIB_DEBUG_PRINTLN_LVL("", __VA_ARGS__)
#define RADIOLIB_DEBUG_SPI_PRINT_FLOAT(...) RADIOLIB_DEBUG_PRINT_FLOAT("RLB_SPI: ", __VA_ARGS__);
#define RADIOLIB_DEBUG_SPI_HEXDUMP(...) RADIOLIB_DEBUG_HEXDUMP("RLB_SPI: ", __VA_ARGS__);
#else
#define RADIOLIB_DEBUG_SPI_PRINT(...) {}
#define RADIOLIB_DEBUG_SPI_PRINT_NOTAG(...) {}
#define RADIOLIB_DEBUG_SPI_PRINTLN(...) {}
#define RADIOLIB_DEBUG_SPI_PRINTLN_NOTAG(...) {}
#define RADIOLIB_DEBUG_SPI_PRINT_FLOAT(...) {}
#define RADIOLIB_DEBUG_SPI_HEXDUMP(...) {}
#endif
// debug info strings
#define RADIOLIB_VALUE_TO_STRING(x) #x
#define RADIOLIB_VALUE(x) RADIOLIB_VALUE_TO_STRING(x)
#define RADIOLIB_INFO "\nRadioLib Info\nVersion: \"" \
RADIOLIB_VALUE(RADIOLIB_VERSION_MAJOR) "." \
RADIOLIB_VALUE(RADIOLIB_VERSION_MINOR) "." \
RADIOLIB_VALUE(RADIOLIB_VERSION_PATCH) "." \
RADIOLIB_VALUE(RADIOLIB_VERSION_EXTRA) "\"\n" \
"Platform: " RADIOLIB_VALUE(RADIOLIB_PLATFORM) "\n" \
"Compiled: " RADIOLIB_VALUE(__DATE__) " " RADIOLIB_VALUE(__TIME__)
#if RADIOLIB_VERBOSE_ASSERT
#define RADIOLIB_ASSERT(STATEVAR) { if((STATEVAR) != RADIOLIB_ERR_NONE) { RADIOLIB_DEBUG_BASIC_PRINTLN("%d at %s:%d", STATEVAR, __FILE__, __LINE__); return(STATEVAR); } }
#else
#define RADIOLIB_ASSERT(STATEVAR) { if((STATEVAR) != RADIOLIB_ERR_NONE) { return(STATEVAR); } }
#endif
#if RADIOLIB_CHECK_PARAMS
#define RADIOLIB_CHECK_RANGE(VAR, MIN, MAX, ERR) { if(!(((VAR) >= (MIN)) && ((VAR) <= (MAX)))) { return(ERR); } }
#else
#define RADIOLIB_CHECK_RANGE(VAR, MIN, MAX, ERR) {}
#endif
#if RADIOLIB_FIX_ERRATA_SX127X
#define RADIOLIB_ERRATA_SX127X(...) { errataFix(__VA_ARGS__); }
#else
#define RADIOLIB_ERRATA_SX127X(...) {}
#endif
// these macros are usually defined by Arduino, but some platforms undef them, so its safer to use our own
#define RADIOLIB_MIN(a,b) ((a)<(b)?(a):(b))
#define RADIOLIB_MAX(a,b) ((a)>(b)?(a):(b))
#define RADIOLIB_ABS(x) ((x)>0?(x):-(x))
// version definitions
#define RADIOLIB_VERSION_MAJOR 7
#define RADIOLIB_VERSION_MINOR 0
#define RADIOLIB_VERSION_PATCH 0
#define RADIOLIB_VERSION_EXTRA 0
#define RADIOLIB_VERSION (((RADIOLIB_VERSION_MAJOR) << 24) | ((RADIOLIB_VERSION_MINOR) << 16) | ((RADIOLIB_VERSION_PATCH) << 8) | (RADIOLIB_VERSION_EXTRA))
#endif
RadioLibTime_t
unsigned long RadioLibTime_t
Type used for durations in RadioLib.
Definition: TypeDef.h:621