# RadioLib: Member List

CC1101 Member List

This is the complete list of members for CC1101, including all inherited members.

autoSetRxBandwidth() | CC1101 |
available() | PhysicalLayer |
begin(float freq=RADIOLIB_CC1101_DEFAULT_FREQ, float br=RADIOLIB_CC1101_DEFAULT_BR, float freqDev=RADIOLIB_CC1101_DEFAULT_FREQDEV, float rxBw=RADIOLIB_CC1101_DEFAULT_RXBW, int8_t pwr=RADIOLIB_CC1101_DEFAULT_POWER, uint8_t preambleLength=RADIOLIB_CC1101_DEFAULT_PREAMBLELEN) | CC1101 |
calculateRxTimeout(RadioLibTime_t timeoutUs) | PhysicalLayer | virtual
CC1101(Module *module) | CC1101 |
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) override | CC1101 | virtual
checkOutputPower(int8_t power, int8_t *clipped, uint8_t *raw) | CC1101 |
clearChannelScanAction() | PhysicalLayer | virtual
clearGdo0Action() | CC1101 |
clearGdo2Action() | CC1101 |
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqFlags(uint32_t irq) | PhysicalLayer | virtual
clearPacketReceivedAction() override | CC1101 | virtual
clearPacketSentAction() override | CC1101 | virtual
disableAddressFiltering() | CC1101 |
disableSyncWordFiltering(bool requireCarrierSense=false) | CC1101 |
dropSync() | PhysicalLayer |
enableSyncWordFiltering(uint8_t maxErrBits=0, bool requireCarrierSense=false) | CC1101 |
finishTransmit() override | CC1101 | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_CC1101_MAX_PACKET_LENGTH) | CC1101 |
getChannelScanResult() | PhysicalLayer | virtual
getChipVersion() | CC1101 |
getFreqStep() const | PhysicalLayer |
getFrequencyDeviation(float *freqDev) | CC1101 |
getIrqFlags() | PhysicalLayer | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getLQI() const | CC1101 |
getPacketLength(bool update=true) override | CC1101 | virtual
getPromiscuousMode() | CC1101 |
getRSSI() override | CC1101 | virtual
getSNR() | PhysicalLayer | virtual
getTimeOnAir(size_t len) | PhysicalLayer | virtual
invertIQ(bool enable) | PhysicalLayer | virtual
packetMode() | CC1101 |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | CC1101 | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | CC1101 | virtual
readData(uint8_t *data, size_t len) override | CC1101 | virtual
readData(uint8_t *data, size_t len) | CC1101 |
receive(uint8_t *data, size_t len) override | CC1101 | virtual
receive(uint8_t *data, size_t len) | CC1101 |
receiveDirect() override | CC1101 | virtual
receiveDirectAsync() | CC1101 |
reset() | CC1101 |
scanChannel() | PhysicalLayer | virtual
scanChannel(ChannelScanConfig_t config) | PhysicalLayer | virtual
setBitRate(float br) override | CC1101 | virtual
setBitRateTolerance(uint8_t brt) | CC1101 |
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setCrcFiltering(bool enable=true) | CC1101 |
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) override | CC1101 | virtual
setDIOMapping(uint32_t pin, uint32_t value) override | CC1101 | virtual
setDirectAction(void(*func)(void)) override | CC1101 | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | CC1101 | virtual
setFrequency(float freq) override | CC1101 | virtual
setFrequencyDeviation(float freqDev) override | CC1101 | virtual
setGdo0Action(void(*func)(void), uint32_t dir) | CC1101 |
setGdo2Action(void(*func)(void), uint32_t dir) | CC1101 |
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqFlags(uint32_t irq) | PhysicalLayer | virtual
setNodeAddress(uint8_t nodeAddr, uint8_t numBroadcastAddrs=0) | CC1101 |
setOOK(bool enableOOK) | CC1101 |
setOutputPower(int8_t pwr) override | CC1101 | virtual
setPacketReceivedAction(void(*func)(void)) override | CC1101 | virtual
setPacketSentAction(void(*func)(void)) override | CC1101 | virtual
setPreambleLength(uint8_t preambleLength, uint8_t qualityThreshold) | CC1101 |
PhysicalLayer::setPreambleLength(size_t len) | PhysicalLayer | virtual
setPromiscuousMode(bool enable=true, bool requireCarrierSense=false) | CC1101 |
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | CC1101 |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | CC1101 |
setRxBandwidth(float rxBw) | CC1101 |
setSyncWord(uint8_t syncH, uint8_t syncL, uint8_t maxErrBits=0, bool requireCarrierSense=false) | CC1101 |
setSyncWord(uint8_t *syncWord, uint8_t len, uint8_t maxErrBits=0, bool requireCarrierSense=false) | CC1101 |
PhysicalLayer::setSyncWord(uint8_t *sync, size_t len) | PhysicalLayer | virtual
sleep() | PhysicalLayer | virtual
standby() override | CC1101 | virtual
standby(uint8_t mode) override | CC1101 | virtual
startChannelScan() | PhysicalLayer | virtual
startChannelScan(const ChannelScanConfig_t &config) | PhysicalLayer | virtual
startDirect() | PhysicalLayer |
startReceive() override | CC1101 | virtual
startReceive(uint32_t timeout, uint32_t irqFlags, uint32_t irqMask, size_t len) override | CC1101 | virtual
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | CC1101 | virtual
startTransmit(const char *str, uint8_t addr=0) | CC1101 |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | CC1101 |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | CC1101 | virtual
transmit(const char *str, uint8_t addr=0) | CC1101 |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | CC1101 |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | CC1101 | virtual
transmitDirectAsync(uint32_t frf=0) | CC1101 |
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_CC1101_MAX_PACKET_LENGTH) | CC1101 |