# RadioLib: Member List

LR1121 Member List

This is the complete list of members for LR1121, including all inherited members.

available() | PhysicalLayer |
begin(float freq=434.0, float bw=125.0, uint8_t sf=9, uint8_t cr=7, uint8_t syncWord=RADIOLIB_LR11X0_LORA_SYNC_WORD_PRIVATE, int8_t power=10, uint16_t preambleLength=8, float tcxoVoltage=1.6) | LR1120 |
LR11x0::begin(float bw, uint8_t sf, uint8_t cr, uint8_t syncWord, uint16_t preambleLength, float tcxoVoltage) | LR11x0 |
beginGFSK(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=156.2, int8_t power=10, uint16_t preambleLength=16, float tcxoVoltage=1.6) | LR1120 |
LR11x0::beginGFSK(float br, float freqDev, float rxBw, uint16_t preambleLength, float tcxoVoltage) | LR11x0 |
beginLRFHSS(float freq=434.0, uint8_t bw=RADIOLIB_LR11X0_LR_FHSS_BW_722_66, uint8_t cr=RADIOLIB_LR11X0_LR_FHSS_CR_2_3, int8_t power=10, float tcxoVoltage=1.6) | LR1120 |
LR11x0::beginLRFHSS(uint8_t bw, uint8_t cr, float tcxoVoltage) | LR11x0 |
calculateRxTimeout(RadioLibTime_t timeoutUs) override | LR11x0 | virtual
checkDataRate(DataRate_t dr) override | LR11x0 | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) override | LR1120 | virtual
checkOutputPower(int8_t power, int8_t *clipped, bool forceHighPower) | LR1120 |
clearChannelScanAction() | PhysicalLayer | virtual
clearIrqAction() | LR11x0 |
clearIrqFlags(uint32_t irq) override | LR11x0 | virtual
clearPacketReceivedAction() override | LR11x0 | virtual
clearPacketSentAction() override | LR11x0 | virtual
clearWiFiScanAction() | LR11x0 |
disableAddressFiltering() | LR11x0 |
dropSync() | PhysicalLayer |
explicitHeader() | LR11x0 |
finishTransmit() override | LR11x0 | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_LR11X0_MAX_PACKET_LENGTH) | LR11x0 |
getChannelScanResult() override | LR11x0 | virtual
getDataRate() const | LR11x0 |
getFreqStep() const | PhysicalLayer |
getFrequencyError() | LR11x0 |
getIrqFlags() override | LR11x0 | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getIrqStatus() | LR11x0 |
getPacketLength(bool update=true) override | LR11x0 | virtual
getPacketLength(bool update, uint8_t *offset) | LR11x0 |
getRSSI() override | LR11x0 | virtual
getSNR() override | LR11x0 | virtual
getTimeOnAir(size_t len) override | LR11x0 | virtual
getVersionInfo(LR11x0VersionInfo_t *info) | LR11x0 |
getWifiScanResult(LR11x0WifiResult_t *result, uint8_t index, bool brief=false) | LR11x0 |
getWifiScanResultsCount(uint8_t *count) | LR11x0 |
implicitHeader(size_t len) | LR11x0 |
invertIQ(bool enable) override | LR11x0 | virtual
LR1120(Module *mod) | LR1120 |
LR1121(Module *mod) | LR1121 |
LR11x0(Module *mod) | LR11x0 | explicit
MODE_END_OF_TABLE enum value | LR11x0 |
MODE_GNSS enum value | LR11x0 |
MODE_RX enum value | LR11x0 |
MODE_STBY enum value | LR11x0 |
MODE_TX enum value | LR11x0 |
MODE_TX_HF enum value | LR11x0 |
MODE_TX_HP enum value | LR11x0 |
MODE_WIFI enum value | LR11x0 |
OpMode_t enum name | LR11x0 |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | LR11x0 | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) | PhysicalLayer | virtual
readData(uint8_t *data, size_t len) override | LR11x0 | virtual
readData(uint8_t *data, size_t len) | LR11x0 |
receive(uint8_t *data, size_t len) override | LR11x0 | virtual
receive(uint8_t *data, size_t len) | LR11x0 |
receiveDirect() override | LR11x0 | virtual
reset() | LR11x0 |
scanChannel() override | LR11x0 | virtual
scanChannel(ChannelScanConfig_t config) override | LR11x0 | virtual
setBandwidth(float bw) | LR11x0 |
setBitRate(float br) override | LR11x0 | virtual
setBroadcastAddress(uint8_t broadAddr) | LR11x0 |
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setCodingRate(uint8_t cr, bool longInterleave=false) | LR11x0 |
setCRC(uint8_t len, uint32_t initial=0x00001D0FUL, uint32_t polynomial=0x00001021UL, bool inverted=true) | LR11x0 |
setDataRate(DataRate_t dr) override | LR11x0 | virtual
setDataShaping(uint8_t sh) override | LR11x0 | virtual
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) | PhysicalLayer | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | LR11x0 | virtual
setFrequency(float freq) override | LR1120 | virtual
setFrequency(float freq, bool calibrate, float band=4) | LR1120 |
setFrequencyDeviation(float freqDev) override | LR11x0 | virtual
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqAction(void(*func)(void)) | LR11x0 |
setIrqFlags(uint32_t irq) override | LR11x0 | virtual
setLrFhssConfig(uint8_t bw, uint8_t cr, uint8_t hdrCount=3, uint16_t hopSeed=0x13A) | LR11x0 |
setNodeAddress(uint8_t nodeAddr) | LR11x0 |
setOutputPower(int8_t power) override | LR1120 | virtual
setOutputPower(int8_t power, bool forceHighPower) | LR1120 |
setPacketReceivedAction(void(*func)(void)) override | LR11x0 | virtual
setPacketSentAction(void(*func)(void)) override | LR11x0 | virtual
setPreambleLength(size_t preambleLength) override | LR11x0 | virtual
setRegulatorDCDC() | LR11x0 |
setRegulatorLDO() | LR11x0 |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | LR11x0 |
setRxBandwidth(float rxBw) | LR11x0 |
setRxBoostedGainMode(bool en) | LR11x0 |
setSpreadingFactor(uint8_t sf, bool legacy=false) | LR11x0 |
setSyncBits(uint8_t *syncWord, uint8_t bitsLen) | LR11x0 |
setSyncWord(uint32_t syncWord) | LR11x0 |
setSyncWord(uint8_t *syncWord, size_t len) override | LR11x0 | virtual
setTCXO(float voltage, uint32_t delay=5000) | LR11x0 |
setWhitening(bool enabled, uint16_t initial=0x01FF) | LR11x0 |
setWiFiScanAction(void(*func)(void)) | LR11x0 |
sleep() override | LR11x0 | virtual
sleep(bool retainConfig, uint32_t sleepTime) | LR11x0 |
standby() override | LR11x0 | virtual
standby(uint8_t mode, bool wakeup=true) | LR11x0 |
PhysicalLayer::standby(uint8_t mode) | PhysicalLayer | virtual
startChannelScan() override | LR11x0 | virtual
startChannelScan(const ChannelScanConfig_t &config) override | LR11x0 | virtual
startDirect() | PhysicalLayer |
startReceive() override | LR11x0 | virtual
startReceive(uint32_t timeout, uint32_t irqFlags=RADIOLIB_LR11X0_IRQ_RX_DONE, uint32_t irqMask=0, size_t len=0) | LR11x0 | virtual
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | LR11x0 | virtual
startTransmit(const char *str, uint8_t addr=0) | LR11x0 |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | LR11x0 |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
startWifiScan(char wifiType, uint8_t mode=RADIOLIB_LR11X0_WIFI_ACQ_MODE_FULL_BEACON, uint16_t chanMask=RADIOLIB_LR11X0_WIFI_ALL_CHANNELS, uint8_t numScans=16, uint16_t timeout=100) | LR11x0 |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | LR11x0 | virtual
transmit(const char *str, uint8_t addr=0) | LR11x0 |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | LR11x0 |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | LR11x0 | virtual
updateFirmware(const uint32_t *image, size_t size, bool nonvolatile=true) | LR11x0 |
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_LR11X0_MAX_PACKET_LENGTH) | LR11x0 |
wifiScan(uint8_t wifiType, uint8_t *count, uint8_t mode=RADIOLIB_LR11X0_WIFI_ACQ_MODE_FULL_BEACON, uint16_t chanMask=RADIOLIB_LR11X0_WIFI_ALL_CHANNELS, uint8_t numScans=16, uint16_t timeout=100) | LR11x0 |
XTAL | LR11x0 |