# RadioLib: Member List

SX127x Member List

This is the complete list of members for SX127x, including all inherited members.

available() | PhysicalLayer |
begin(uint8_t *chipVersions, uint8_t numVersions, uint8_t syncWord, uint16_t preambleLength) | SX127x |
beginFSK(uint8_t *chipVersions, uint8_t numVersions, float freqDev, float rxBw, uint16_t preambleLength, bool enableOOK) | SX127x |
calculateRxTimeout(RadioLibTime_t timeoutUs) override | SX127x | virtual
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) | PhysicalLayer | virtual
clearChannelScanAction() override | SX127x | virtual
clearDio0Action() | SX127x |
clearDio1Action() | SX127x |
clearFHSSInt(void) | SX127x |
clearFifoEmptyAction() | SX127x |
clearFifoFullAction() | SX127x |
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqFlags(uint32_t irq) override | SX127x | virtual
clearPacketReceivedAction() override | SX127x | virtual
clearPacketSentAction() override | SX127x | virtual
disableAddressFiltering() | SX127x |
disableBitSync() | SX127x |
dropSync() | PhysicalLayer |
enableBitSync() | SX127x |
fifoAdd(uint8_t *data, int totalLen, int *remLen) | SX127x |
fifoGet(volatile uint8_t *data, int totalLen, volatile int *rcvLen) | SX127x |
finishTransmit() override | SX127x | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_SX127X_MAX_PACKET_LENGTH_FSK) | SX127x |
getAFCError() | SX127x |
getChannelScanResult() override | SX127x | virtual
getChipVersion() | SX127x |
getDataRate() const | SX127x |
getFHSSChannel(void) | SX127x |
getFHSSHoppingPeriod(void) | SX127x |
getFreqStep() const | PhysicalLayer |
getFrequencyError(bool autoCorrect=false) | SX127x |
getIrqFlags() override | SX127x | virtual
getIRQFlags() | SX127x |
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getModemStatus() | SX127x |
getNumSymbols(size_t len) | SX127x |
getPacketLength(bool update=true) override | SX127x | virtual
PhysicalLayer::getRSSI() | PhysicalLayer | virtual
getSNR() override | SX127x | virtual
getTempRaw() | SX127x |
getTimeOnAir(size_t len) override | SX127x | virtual
invertIQ(bool enable) override | SX127x | virtual
invertPreamble(bool enable) | SX127x |
packetMode() | SX127x |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | SX127x | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | SX127x | virtual
readData(uint8_t *data, size_t len) override | SX127x | virtual
readData(uint8_t *data, size_t len) | SX127x |
receive(uint8_t *data, size_t len) override | SX127x | virtual
receive(uint8_t *data, size_t len) | SX127x |
receiveDirect() override | SX127x | virtual
reset()=0 | SX127x | pure virtual
scanChannel() override | SX127x | virtual
PhysicalLayer::scanChannel(ChannelScanConfig_t config) | PhysicalLayer | virtual
setAFC(bool isEnabled) | SX127x |
setAFCAGCTrigger(uint8_t trigger) | SX127x |
setAFCBandwidth(float afcBw) | SX127x |
setBitRate(float br) | PhysicalLayer | virtual
setBroadcastAddress(uint8_t broadAddr) | SX127x |
setChannelScanAction(void(*func)(void)) override | SX127x | virtual
setCrcFiltering(bool enable=true) | SX127x |
setCurrentLimit(uint8_t currentLimit) | SX127x |
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) | PhysicalLayer | virtual
setDio0Action(void(*func)(void), uint32_t dir) | SX127x |
setDio1Action(void(*func)(void), uint32_t dir) | SX127x |
setDIOMapping(uint32_t pin, uint32_t value) override | SX127x | virtual
setDIOPreambleDetect(bool usePreambleDetect) | SX127x |
setDirectAction(void(*func)(void)) override | SX127x | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | SX127x | virtual
setFHSSHoppingPeriod(uint8_t freqHoppingPeriod) | SX127x |
setFifoEmptyAction(void(*func)(void)) | SX127x |
setFifoFullAction(void(*func)(void)) | SX127x |
setFrequency(float freq) | PhysicalLayer | virtual
setFrequencyDeviation(float freqDev) override | SX127x | virtual
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqFlags(uint32_t irq) override | SX127x | virtual
setLowBatteryThreshold(int8_t level, uint32_t pin=RADIOLIB_NC) | SX127x |
setNodeAddress(uint8_t nodeAddr) | SX127x |
setOOK(bool enableOOK) | SX127x |
setOokFixedOrFloorThreshold(uint8_t value) | SX127x |
setOokPeakThresholdDecrement(uint8_t value) | SX127x |
setOokPeakThresholdStep(uint8_t value) | SX127x |
setOokThresholdType(uint8_t type) | SX127x |
setOutputPower(int8_t power) | PhysicalLayer | virtual
setPacketReceivedAction(void(*func)(void)) override | SX127x | virtual
setPacketSentAction(void(*func)(void)) override | SX127x | virtual
setPreambleLength(size_t preambleLength) override | SX127x | virtual
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | SX127x |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | SX127x |
setRSSIConfig(uint8_t smoothingSamples, int8_t offset=0) | SX127x |
setRSSIThreshold(float dbm) | SX127x |
setRxBandwidth(float rxBw) | SX127x |
setSyncWord(uint8_t syncWord) | SX127x |
setSyncWord(uint8_t *syncWord, size_t len) override | SX127x | virtual
sleep() override | SX127x | virtual
standby() override | SX127x | virtual
standby(uint8_t mode) override | SX127x | virtual
startChannelScan() override | SX127x | virtual
PhysicalLayer::startChannelScan(const ChannelScanConfig_t &config) | PhysicalLayer | virtual
startDirect() | PhysicalLayer |
startReceive() override | SX127x | virtual
startReceive(uint32_t timeout, RadioLibIrqFlags_t irqFlags=RADIOLIB_IRQ_RX_DEFAULT_FLAGS, RadioLibIrqFlags_t irqMask=RADIOLIB_IRQ_RX_DEFAULT_MASK, size_t len=0) override | SX127x | virtual
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX127x | virtual
startTransmit(const char *str, uint8_t addr=0) | SX127x |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX127x |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
SX127x(Module *mod) | SX127x | explicit
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | SX127x | virtual
transmit(const char *str, uint8_t addr=0) | SX127x |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | SX127x |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | SX127x | virtual
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_SX127X_MAX_PACKET_LENGTH_FSK) | SX127x |