# RadioLib: Member List

Si4430 Member List

This is the complete list of members for Si4430, including all inherited members.

available() | PhysicalLayer |
begin(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=181.1, int8_t power=10, uint8_t preambleLen=16) | Si4430 |
Si443x::begin(float br, float freqDev, float rxBw, uint8_t preambleLen) | Si443x |
calculateRxTimeout(RadioLibTime_t timeoutUs) | PhysicalLayer | virtual
checkDataRate(DataRate_t dr) | PhysicalLayer | virtual
checkIrq(RadioLibIrqType_t irq) | PhysicalLayer |
checkOutputPower(int8_t power, int8_t *clipped) | PhysicalLayer | virtual
clearChannelScanAction() | PhysicalLayer | virtual
clearIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
clearIrqAction() | Si443x |
clearIrqFlags(uint32_t irq) | PhysicalLayer | virtual
clearPacketReceivedAction() override | Si443x | virtual
clearPacketSentAction() override | Si443x | virtual
dropSync() | PhysicalLayer |
finishTransmit() override | Si443x | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_SI443X_MAX_PACKET_LENGTH) | Si443x |
getChannelScanResult() | PhysicalLayer | virtual
getChipVersion() | Si443x |
getFreqStep() const | PhysicalLayer |
getIrqFlags() | PhysicalLayer | virtual
getIrqMapped(RadioLibIrqFlags_t irq) | PhysicalLayer |
getPacketLength(bool update=true) override | Si443x | virtual
getRSSI() | PhysicalLayer | virtual
getSNR() | PhysicalLayer | virtual
getTimeOnAir(size_t len) | PhysicalLayer | virtual
invertIQ(bool enable) | PhysicalLayer | virtual
packetMode() | Si443x |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | Si443x | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | Si443x | virtual
readData(uint8_t *data, size_t len) override | Si443x | virtual
readData(uint8_t *data, size_t len) | Si443x |
receive(uint8_t *data, size_t len) override | Si443x | virtual
receive(uint8_t *data, size_t len) | Si443x |
receiveDirect() override | Si443x | virtual
reset() | Si443x |
scanChannel() | PhysicalLayer | virtual
scanChannel(ChannelScanConfig_t config) | PhysicalLayer | virtual
setBitRate(float br) override | Si443x | virtual
setChannelScanAction(void(*func)(void)) | PhysicalLayer | virtual
setDataRate(DataRate_t dr) | PhysicalLayer | virtual
setDataShaping(uint8_t sh) override | Si443x | virtual
setDIOMapping(uint32_t pin, uint32_t value) | PhysicalLayer | virtual
setDirectAction(void(*func)(void)) override | Si443x | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | Si443x | virtual
setFrequency(float freq) override | Si4430 | virtual
setFrequencyDeviation(float freqDev) override | Si443x | virtual
setIrq(RadioLibIrqFlags_t irq) | PhysicalLayer |
setIrqAction(void(*func)(void)) | Si443x |
setIrqFlags(uint32_t irq) | PhysicalLayer | virtual
setOutputPower(int8_t power) override | Si4430 | virtual
setPacketReceivedAction(void(*func)(void)) override | Si443x | virtual
setPacketSentAction(void(*func)(void)) override | Si443x | virtual
setPreambleLength(uint8_t preambleLen) | Si443x |
PhysicalLayer::setPreambleLength(size_t len) | PhysicalLayer | virtual
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | Si443x |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | Si443x |
setRxBandwidth(float rxBw) | Si443x |
setSyncWord(uint8_t *syncWord, size_t len) override | Si443x | virtual
Si4430(Module *mod) | Si4430 |
Si4432(Module *mod) | Si4432 |
Si443x(Module *mod) | Si443x | explicit
sleep() override | Si443x | virtual
standby() override | Si443x | virtual
standby(uint8_t mode) override | Si443x | virtual
startChannelScan() | PhysicalLayer | virtual
startChannelScan(const ChannelScanConfig_t &config) | PhysicalLayer | virtual
startDirect() | PhysicalLayer |
startReceive() override | Si443x | virtual
startReceive(uint32_t timeout, uint32_t irqFlags, uint32_t irqMask, size_t len) override | Si443x | virtual
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) override | Si443x | virtual
startTransmit(const char *str, uint8_t addr=0) | Si443x |
startTransmit(const uint8_t *data, size_t len, uint8_t addr=0) | Si443x |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) override | Si443x | virtual
transmit(const char *str, uint8_t addr=0) | Si443x |
transmit(const uint8_t *data, size_t len, uint8_t addr=0) | Si443x |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | Si443x | virtual
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_SI443X_MAX_PACKET_LENGTH) | Si443x |