From 0d1194aaf2b2ebc571cf01d2353d252c12146d2e Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Mon, 27 Jun 2016 16:08:26 +0200
Subject: [PATCH 10/82] ARM: dts: sun8i-h3: Add clock-frequency

To avoid error messages during boot.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-h3.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-h3.dtsi b/arch/arm/boot/dts/sun8i-h3.dtsi
index f0096074a467..cb19ff797606 100644
--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -78,6 +78,7 @@
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
 			#cooling-cells = <2>;
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@1 {
@@ -88,6 +89,7 @@
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
 			#cooling-cells = <2>;
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@2 {
@@ -98,6 +100,7 @@
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
 			#cooling-cells = <2>;
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@3 {
@@ -108,6 +111,7 @@
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
 			#cooling-cells = <2>;
+			clock-frequency = <1200000000>;
 		};
 	};
 
-- 
2.20.1

