diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
index f1fc6bdca..47a5635b0 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
@@ -129,6 +129,10 @@
 	status = "okay";
 };
 
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpux>;
+};
+
 &ehci1 {
 	status = "okay";
 };
@@ -179,6 +183,31 @@
 	};
 };
 
+&r_i2c {
+	status = "okay";
+
+	reg_vdd_cpux: regulator@65 {
+		compatible = "silergy,sy8106a";
+		reg = <0x65>;
+		regulator-name = "vdd-cpux";
+		silergy,fixed-microvolt = <1200000>;
+		/*
+		 * The datasheet uses 1.1V as the minimum value of VDD-CPUX,
+		 * however both the Armbian DVFS table and the official one
+		 * have operating points with voltage under 1.1V, and both
+		 * DVFS table are known to work properly at the lowest
+		 * operating point.
+		 *
+		 * Use 1.0V as the minimum voltage instead.
+		 */
+		regulator-min-microvolt = <1000000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-ramp-delay = <200>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+}; 
+
 &pio {
 	leds_opc: led_pins {
 		pins = "PA15";
