From 4e3d17aa91541ce9ad705432e6ef353efabeb06e Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sat, 25 Jun 2016 00:02:04 +0200
Subject: [PATCH 06/82] dt-bindings: document sun8i_ths - H3 thermal sensor
 driver
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch adds the binding documentation for the
sun8i_ths driver. This is a driver for thermal sensor
found in Allwinner H3 SoC.

Signed-off-by: Ondřej Jirman <megous@megous.com>
---
 .../devicetree/bindings/thermal/sun8i-ths.txt | 24 +++++++++++++++++++
 1 file changed, 24 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/thermal/sun8i-ths.txt

diff --git a/Documentation/devicetree/bindings/thermal/sun8i-ths.txt b/Documentation/devicetree/bindings/thermal/sun8i-ths.txt
new file mode 100644
index 000000000000..ba1288165e90
--- /dev/null
+++ b/Documentation/devicetree/bindings/thermal/sun8i-ths.txt
@@ -0,0 +1,24 @@
+* Thermal sensor driver for Allwinner H3 SoC
+
+Required properties:
+- compatible : "allwinner,sun8i-h3-ths"
+- reg : Address range of the thermal sensor registers
+- resets : Must contain phandles to reset controls matching the entries
+  of the names
+- reset-names : Must include the name "ahb"
+- clocks : Must contain phandles to clock controls matching the entries
+  of the names
+- clock-names : Must contain "ahb" for the bus gate and "ths" for the THS
+  clock
+
+Example:
+ths: ths@01c25000 {
+	#thermal-sensor-cells = <0>;
+	compatible = "allwinner,sun8i-h3-ths";
+	reg = <0x01c25000 0x400>;
+	interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
+	resets = <&bus_rst 136>;
+	reset-names = "ahb";
+	clocks = <&bus_gates 72>, <&ths_clk>;
+	clock-names = "ahb", "ths";
+};
-- 
2.20.1

