diff --git a/configs/orangepi_win_defconfig b/configs/orangepi_win_defconfig
index a3e278f..39e83f1 100644
--- a/configs/orangepi_win_defconfig
+++ b/configs/orangepi_win_defconfig
@@ -12,6 +12,9 @@ CONFIG_SPL=y
 # CONFIG_SPL_ISO_PARTITION is not set
 # CONFIG_SPL_EFI_PARTITION is not set
 CONFIG_SPL_SPI_SUNXI=y
+CONFIG_SPL_SPI_FLASH_SUPPORT=y
+CONFIG_USB1_VBUS_PIN="PD7"
+CONFIG_USB_HOST=y
 CONFIG_SUN8I_EMAC=y
 CONFIG_USB_EHCI_HCD=y
 CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
diff --git a/arch/arm/dts/sun50i-a64-orangepi-win.dts b/arch/arm/dts/sun50i-a64-orangepi-win.dts
index cf76c35..a7d36a5 100644
--- a/arch/arm/dts/sun50i-a64-orangepi-win.dts
+++ b/arch/arm/dts/sun50i-a64-orangepi-win.dts
@@ -64,6 +64,19 @@
 		regulator-min-microvolt = <3300000>;
 		regulator-max-microvolt = <3300000>;
 	};
+
+	reg_usb1_vbus: usb1-vbus {
+		compatible = "regulator-fixed";
+		pinctrl-names = "default";
+		pinctrl-0 = <&usb1_vbus_pin_opiwin>;
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 7 GPIO_ACTIVE_HIGH>;
+		status = "okay";
+	};
 };
 
 &ehci1 {
@@ -83,6 +96,13 @@
        status = "okay";
 };
 
+&pio {
+	usb1_vbus_pin_opiwin: usb1_vbus_pin@0 {
+		allwinner,pins = "PD7";
+		allwinner,function = "gpio_out";
+	};
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
@@ -90,5 +112,6 @@
 };
 
 &usbphy {
-       status = "okay";
+	usb1_vbus-supply = <&reg_usb1_vbus>;
+	status = "okay";
 };
