From d9ad129ac7a3114568a323f44316d9d5bfd9a3f9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Myl=C3=A8ne=20Josserand?= <mylene.josserand@bootlin.com>
Date: Mon, 5 Mar 2018 11:04:31 +0100
Subject: [PATCH 39/60] ARM: dts: sun8i: Add the H3/H5 CSI controller
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The H3 and H5 features the same CSI controller that was initially found on
the A31.

Add a DT node for it.

Signed-off-by: Mylène Josserand <mylene.josserand@bootlin.com>
Signed-off-by: Maxime Ripard <maxime.ripard@bootlin.com>
---
 arch/arm/boot/dts/sunxi-h3-h5.dtsi            | 22 +++++++++++++++++++
 .../platform/sunxi/sun6i-csi/sun6i_csi.c      |  1 +
 2 files changed, 23 insertions(+)

diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index ff05c532792d..be75e7cfdc3a 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -550,6 +550,13 @@
 			interrupt-controller;
 			#interrupt-cells = <3>;
 
+			csi_pins: csi {
+				pins = "PE0", "PE1", "PE2", "PE3", "PE4",
+				       "PE5", "PE6", "PE7", "PE8", "PE9",
+				       "PE10", "PE11";
+				function = "csi";
+			};
+
 			emac_rgmii_pins: emac0 {
 				pins = "PD0", "PD1", "PD2", "PD3", "PD4",
 				       "PD5", "PD7", "PD8", "PD9", "PD10",
@@ -936,6 +943,21 @@
 			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
 		};
 
+		csi: camera@1cb0000 {
+			compatible = "allwinner,sun8i-h3-csi",
+				     "allwinner,sun6i-a31-csi";
+			reg = <0x01cb0000 0x1000>;
+			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_CSI>,
+				 <&ccu CLK_CSI_SCLK>,
+				 <&ccu CLK_DRAM_CSI>;
+			clock-names = "bus", "mod", "ram";
+			resets = <&ccu RST_BUS_CSI>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&csi_pins>;
+			status = "disabled";
+		};
+
 		rtc: rtc@1f00000 {
 			compatible = "allwinner,sun6i-a31-rtc";
 			reg = <0x01f00000 0x54>;

-- 
2.20.1
