diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index afed6c0dea6f..798ab48c5479 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -992,6 +992,19 @@
 			reg = <0x1f01c00 0x400>;
 		};
 
+		r_cir: ir@1f02000 {
+			compatible = "allwinner,sun8i-a83t-ir",
+				"allwinner,sun5i-a13-ir";
+			clocks = <&r_ccu CLK_APB0_IR>, <&r_ccu CLK_IR>;
+			clock-names = "apb", "ir";
+			resets = <&r_ccu RST_APB0_IR>;
+			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
+			reg = <0x01f02000 0x400>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&r_cir_pin>;
+			status = "disabled";
+		};
+
 		r_pio: pinctrl@1f02c00 {
 			compatible = "allwinner,sun8i-a83t-r-pinctrl";
 			reg = <0x01f02c00 0x400>;
