diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
index 9f33f6fae..561182a9f 100644
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
@@ -47,6 +47,23 @@
 	compatible = "friendlyarm,nanopi-neo", "allwinner,sun8i-h3";
 };
 
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&mmc2_8bit_pins {
+	/* Increase drive strength for DDR modes */
+	drive-strength = <40>;
+	/* eMMC is missing pull-ups */
+	bias-pull-up;
+};
+
 &ehci0 {
 	status = "okay";
 };
