diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index d1890797c..6cb02c962 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -1045,28 +1045,74 @@
 	};
 
 	thermal-zones {
-		cpu_thermal: cpu_thermal {
-			polling-delay-passive = <330>;
+		cpu-thermal {
+			/* milliseconds */
+			polling-delay-passive = <250>;
 			polling-delay = <1000>;
-			thermal-sensors = <&ths 0>;
+			thermal-sensors = <&ths>;
 
 			trips {
-				cpu_hot_trip: cpu-warm {
-					temperature = <65000>;
+				cpu_warm: cpu_warm {
+					temperature = <75000>;
 					hysteresis = <2000>;
 					type = "passive";
 				};
-				cpu_very_hot_trip: cpu-very-hot {
+
+				cpu_hot_pre: cpu_hot_pre {
+					temperature = <80000>;
+					hysteresis = <2000>;
+					type = "passive";
+				};
+
+				cpu_hot: cpu_hot {
+					temperature = <85000>;
+					hysteresis = <2000>;
+					type = "passive";
+				};
+
+				cpu_very_hot_pre: cpu_very_hot_pre {
 					temperature = <90000>;
 					hysteresis = <2000>;
+					type = "passive";
+				};
+
+				cpu_very_hot: cpu_very_hot {
+					temperature = <95000>;
+					hysteresis = <2000>;
+					type = "passive";
+				};
+
+				cpu_crit: cpu_crit {
+					temperature = <105000>;
+					hysteresis = <2000>;
 					type = "critical";
 				};
 			};
 
 			cooling-maps {
-				cpu-warm-limit {
-					trip = <&cpu_hot_trip>;
-					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+				cpu_warm_limit_cpu {
+					trip = <&cpu_warm>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT 2>;
+				};
+
+				cpu_hot_pre_limit_cpu {
+					trip = <&cpu_hot_pre>;
+					cooling-device = <&cpu0 2 3>;
+				};
+
+				cpu_hot_limit_cpu {
+					trip = <&cpu_hot>;
+					cooling-device = <&cpu0 3 4>;
+				};
+
+				cpu_very_hot_pre_limit_cpu {
+					trip = <&cpu_very_hot_pre>;
+					cooling-device = <&cpu0 5 6>;
+				};
+
+				cpu_very_hot_limit_cpu {
+					trip = <&cpu_very_hot>;
+					cooling-device = <&cpu0 7 THERMAL_NO_LIMIT>;
 				};
 			};
 		};
