From 69c8e0651bb68ab80b0fc4033b8ca5e87b8bb164 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Fri, 10 Nov 2017 13:20:43 +0100
Subject: [PATCH 39/82] ARM: dts: sun8i-a83t-tbs-a711: Enable BMA250
 accelerometer IIO

It's already supported in mainline kernel.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index 8e9f0de3d0c0..2427bf3461d7 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -242,6 +242,14 @@
 	pinctrl-0 = <&i2c1_pins>;
 	clock-frequency = <400000>;
 	status = "okay";
+
+	/* Accelerometer */
+	bma250@18 {
+		compatible = "bosch,bma250";
+		reg = <0x18>;
+		interrupt-parent = <&pio>;
+		interrupts = <7 10 IRQ_TYPE_EDGE_RISING>; /* PH10 / EINT10 */
+	};
 };
 
 &mmc0 {
-- 
2.20.1

