From b093d275ba1bec4d8ee91f18609ef0266fa5cbbb Mon Sep 17 00:00:00 2001
From: Sebastian Panceac <sebastian@balena.io>
Date: Wed, 27 Feb 2019 10:13:31 +0100
Subject: [PATCH] Enable uart3 for NanoPi Neo Air used by BT

Upstream-status: Pending
Signed-off-by: Sebastian Panceac <sebastian@balena.io>
---
 arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts | 6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
index 6246d3eff39d..2fc601a0ec82 100644
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
@@ -109,6 +109,12 @@
 	status = "okay";
 };
 
+&uart3 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart3_pins>, <&uart3_rts_cts_pins>;
+	status = "okay";
+};
+
 &usbphy {
 	/* USB VBUS is always on */
 	status = "okay";
-- 
2.17.1

