diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
index 8b93f5c..9011356 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
@@ -51,6 +51,11 @@
 		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
 		ethernet1 = &rtl8189ftv;
 	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 WIFI_EN */
+	};
 };
 
 &mmc1 {
@@ -57,6 +57,7 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc1_pins_a>;
 	vmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
 	bus-width = <4>;
 	non-removable;
 	status = "okay";
