diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
index e1ee1cd09..522a08d6c 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
@@ -1,5 +1,6 @@
 /*
  * Copyright (C) 2017 Jagan Teki <jteki@openedev.com>
+ * Copyright (C) 2019 Adopted by Igor <igor@armbian.com>
  *
  * This file is dual-licensed: you can use it either under the terms
  * of the GPL or the X11 license, at your option. Note that this dual
@@ -180,3 +181,12 @@
 	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
 	status = "okay";
 };
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	status = "okay";
+};
