diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index d3daf90a8715..934d7e87fa08 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -134,6 +134,7 @@
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
 			#cooling-cells = <2>;
+			next-level-cache = <&L2>;
 		};
 
 		cpu1: cpu@1 {
@@ -142,6 +143,7 @@
 			reg = <1>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
+			next-level-cache = <&L2>;
 		};
 
 		cpu2: cpu@2 {
@@ -150,6 +152,7 @@
 			reg = <2>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
+			next-level-cache = <&L2>;
 		};
 
 		cpu3: cpu@3 {
@@ -158,7 +161,13 @@
 			reg = <3>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
+			next-level-cache = <&L2>;
 		};
+		
+		L2: l2-cache {
+			compatible = "cache";
+			cache-level = <2>;
+ 		};
 	};
 
 	de: display-engine {
