We start to get to the limit of our main U-Boot binary size (with some
boards even crossing it). Enable its build using thumb2 to get some extra
room.

Suggested-by: Siarhei Siamashka <siarhei.siamashka at gmail.com>
Signed-off-by: Maxime Ripard <maxime.ripard at free-electrons.com>
---
 arch/arm/Kconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/Kconfig b/arch/arm/Kconfig
index 64e0ee43f112..83b7aa51dc2c 100644
--- a/arch/arm/Kconfig
+++ b/arch/arm/Kconfig
@@ -698,6 +698,7 @@ config ARCH_SUNXI
 	select SPL_SYS_MALLOC_SIMPLE if SPL
 	select SYS_NS16550
 	select SPL_SYS_THUMB_BUILD if !ARM64
+	select SYS_THUMB_BUILD if !ARM64
 	select USB if DISTRO_DEFAULTS
 	select USB_STORAGE if DISTRO_DEFAULTS
 	select USB_KEYBOARD if DISTRO_DEFAULTS
-- 
2.14.2
