From ac8826aeb1f157a76b1f1d31b13eb557d3f96108 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sat, 30 Sep 2017 02:53:26 +0200
Subject: [PATCH 32/82] ARM: dts: sun8i-a83t-tbs-a711: Force dvdd-csi-r/f
 regulators to 1.8V

This is required by camera sensors that are connected to them.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index bd7e231e3aba..7936405862c1 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -353,7 +353,7 @@
 };
 
 &reg_eldo1 {
-	regulator-min-microvolt = <1200000>;
+	regulator-min-microvolt = <1800000>;
 	regulator-max-microvolt = <1800000>;
 	regulator-name = "dvdd-csi-r";
 };
@@ -365,7 +365,7 @@
 };
 
 &reg_eldo3 {
-	regulator-min-microvolt = <1200000>;
+	regulator-min-microvolt = <1800000>;
 	regulator-max-microvolt = <1800000>;
 	regulator-name = "dvdd-csi-f";
 };
-- 
2.20.1

