From a1d32a812faa375b9234e215d46383dd3a3ae377 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Sat, 23 Dec 2017 10:46:45 +0800
Subject: [PATCH 18/35] arm64: allwinner: h6: enable AXP805 PMIC on Pine H64

Pine H64 board has an AXP805 PMIC on it.

Enable it in the device tree.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 .../boot/dts/allwinner/sun50i-h6-pine-h64.dts      | 115 +++++++++++++++++++++
 1 file changed, 115 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts
index 3e31f39..9177224 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-pine-h64.dts
@@ -55,6 +55,121 @@
 	status = "okay";
 };

+&r_i2c {
+	pinctrl-names = "default";
+	pinctrl-0 = <&r_i2c_pins>;
+	status = "okay";
+
+	axp805: pmic@36 {
+		compatible = "x-powers,axp805", "x-powers,axp806";
+		reg = <0x36>;
+		interrupt-parent = <&r_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-controller;
+		#interrupt-cells = <1>;
+		x-powers,master-mode;
+
+		regulators {
+			reg_aldo1: aldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-pl";
+			};
+
+			reg_aldo2: aldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-ac200";
+			};
+
+			reg_aldo3: aldo3 {
+				/* This regulator is connected with CLDO1 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-1";
+			};
+
+			reg_bldo1: bldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-ddr-bias-pll";
+			};
+
+			reg_bldo2: bldo2 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-efuse-emmc-pcie-hdmi";
+			};
+
+			reg_bldo3: bldo3 {
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-wifi-io";
+			};
+
+			bldo4 {
+				/* unused */
+			};
+
+			reg_cldo1: cldo1 {
+				/* This regulator is connected with ALDO3 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-2";
+			};
+
+			reg_cldo2: cldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-1";
+			};
+
+			reg_cldo3: cldo3 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-2";
+			};
+
+			reg_dcdca: dcdca {
+				regulator-always-on;
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1080000>;
+				regulator-name = "vdd-cpu";
+			};
+
+			reg_dcdcc: dcdcc {
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1080000>;
+				regulator-name = "vdd-gpu";
+			};
+
+			reg_dcdcd: dcdcd {
+				regulator-always-on;
+				regulator-min-microvolt = <960000>;
+				regulator-max-microvolt = <960000>;
+				regulator-name = "vdd-sys";
+			};
+
+			reg_dcdce: dcdce {
+				regulator-always-on;
+				regulator-min-microvolt = <1200000>;
+				regulator-max-microvolt = <1200000>;
+				regulator-name = "vcc-dram";
+			};
+
+			sw {
+				/* unused */
+			};
+		};
+	};
+
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_ph_pins>;
--
2.7.4

