From 3d017794525d830a3251bed7ebbacbf74efe9605 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Thu, 18 Oct 2018 15:33:24 +0800
Subject: [PATCH 131/146] arm64: allwinner: a64: add pinmux for RGB666 LCD

Allwinner A64's TCON0 can output RGB666 LCD signal.

Add its pinmux.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 9 +++++++++
 1 file changed, 9 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index cb7d4a96e789..0f5b412cfc81 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -655,6 +655,15 @@
 				function = "i2c1";
 			};
 
+			lcd_rgb666_pins: lcd-rgb666 {
+				pins = "PD0", "PD1", "PD2", "PD3", "PD4",
+				       "PD5", "PD6", "PD7", "PD8", "PD9",
+				       "PD10", "PD11", "PD12", "PD13",
+				       "PD14", "PD15", "PD16", "PD17",
+				       "PD18", "PD19", "PD20", "PD21";
+				function = "lcd0";
+			};
+
 			mmc0_pins: mmc0-pins {
 				pins = "PF0", "PF1", "PF2", "PF3",
 				       "PF4", "PF5";
-- 
2.17.1

