diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
index 5e3dc2666d0f..feb8c7e51623 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
@@ -59,6 +59,15 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	leds {
+		compatible = "gpio-leds";
+
+		blue {
+			label = "nanopi-a64:blue:status";
+			gpios = <&pio 3 24 GPIO_ACTIVE_LOW>; /* PD24 */
+		};
+	};
+
 	wifi_pwrseq: wifi_pwrseq {
 		compatible = "mmc-pwrseq-simple";
 		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
