diff --git a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
index 8da939a..42fd205 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -56,6 +56,7 @@
 
 	aliases {
 		serial0 = &uart0;
+		serial2 = &uart2;
 	};
 
 	chosen {
@@ -307,6 +308,12 @@
 	status = "okay";
 };
 
+&uart2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart2_pins_a>;
+	status = "okay";
+};
+
 &usb_otg {
 	dr_mode = "otg";
 	status = "okay";
