From 6328da39df61f962190870089aaa171a7f8aab2c Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Thu, 30 Mar 2017 13:04:25 +0200
Subject: [PATCH 11/82] arm64: dts: sun50i-h5: Add clock-frequency

To avoid error messages during boot.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
index 62d646baac3c..4452ab873dec 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -52,6 +52,7 @@
 			device_type = "cpu";
 			reg = <0>;
 			enable-method = "psci";
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@1 {
@@ -59,6 +60,7 @@
 			device_type = "cpu";
 			reg = <1>;
 			enable-method = "psci";
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@2 {
@@ -66,6 +68,7 @@
 			device_type = "cpu";
 			reg = <2>;
 			enable-method = "psci";
+			clock-frequency = <1200000000>;
 		};
 
 		cpu@3 {
@@ -73,6 +76,7 @@
 			device_type = "cpu";
 			reg = <3>;
 			enable-method = "psci";
+			clock-frequency = <1200000000>;
 		};
 	};
 
-- 
2.20.1

