From f8b601516e29a67496d98414b2477928d79eb3eb Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 12 Dec 2017 16:15:26 +0100
Subject: [PATCH 65/82] arm: dts: sun8i-a83t-tbs-a711: GPS regulator is
 apparently fixed

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index 028dd29e13d7..027c6a76627f 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -127,7 +127,9 @@
 		regulator-min-microvolt = <3000000>;
 		regulator-max-microvolt = <3000000>;
 		enable-active-high;
-		gpio = <&pio 3 4 GPIO_ACTIVE_HIGH>; /* PD4 */
+		/*XXX: this doesn't control GPS regulator, shematics show FLAG
+		 * pin */
+		//gpio = <&pio 3 4 GPIO_ACTIVE_HIGH>; /* PD4 */
 	};
 
 	reg_vbat: reg-vbat {
-- 
2.20.1

