From 7794e4fa9fa31ac5cb6d7712d76730fc42f21b85 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Wed, 10 Jan 2018 00:02:24 +0800
Subject: [PATCH 33/35] net: stmmac: sun8i: add support for Allwinner H6 EMAC

The EMAC on Allwinner H6 is just like the one on A64. The "internal PHY"
on H6 is on a co-packaged AC200 chip, and it's not really internal (it's
connected via RMII at PA GPIO bank).

Add support for the Allwinner H6 EMAC in the dwmac-sun8i driver.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 Documentation/devicetree/bindings/net/dwmac-sun8i.txt |  2 ++
 drivers/net/ethernet/stmicro/stmmac/dwmac-sun8i.c     | 14 ++++++++++++++
 2 files changed, 16 insertions(+)

diff --git a/drivers/net/ethernet/stmicro/stmmac/dwmac-sun8i.c b/drivers/net/ethernet/stmicro/stmmac/dwmac-sun8i.c
index 099daef..0b3e686 100644
--- a/drivers/net/ethernet/stmicro/stmmac/dwmac-sun8i.c
+++ b/drivers/net/ethernet/stmicro/stmmac/dwmac-sun8i.c
@@ -105,6 +105,18 @@ static const struct emac_variant emac_variant_a64 = {
 	.support_rgmii = true
 };
 
+static const struct emac_variant emac_variant_h6 = {
+	.default_syscon_value = 0x148000,
+	/*
+	 * The "Internal PHY" of H6 is not on the die. It's on the co-packaged
+	 * AC200 chip instead.
+	 */
+	.soc_has_internal_phy = false,
+	.support_mii = true,
+	.support_rmii = true,
+	.support_rgmii = true
+};
+
 #define EMAC_BASIC_CTL0 0x00
 #define EMAC_BASIC_CTL1 0x04
 #define EMAC_INT_STA    0x08
@@ -1085,6 +1097,8 @@ static const struct of_device_id sun8i_dwmac_match[] = {
 		.data = &emac_variant_a83t },
 	{ .compatible = "allwinner,sun50i-a64-emac",
 		.data = &emac_variant_a64 },
+	{ .compatible = "allwinner,sun50i-h6-emac",
+		.data = &emac_variant_h6 },
 	{ }
 };
 MODULE_DEVICE_TABLE(of, sun8i_dwmac_match);
-- 
2.7.4

