From 3ef8fd9d164316d26eb99afec111e0431c2f2c69 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sun, 13 May 2018 21:00:43 +0200
Subject: [PATCH 09/82] ARM: dts: sun8i: Increase max CPUX voltage to 1.4V on
 Orange Pi PC

When using thermal regulation we can afford to go higher. Also add
regulator-ramp-delay, because regulator takes some time to change
voltage.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
index 46240334128f..83f1866ed9e7 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
@@ -204,7 +204,8 @@
 		 * Use 1.0V as the minimum voltage instead.
 		 */
 		regulator-min-microvolt = <1000000>;
-		regulator-max-microvolt = <1300000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-ramp-delay = <200>;
 		regulator-boot-on;
 		regulator-always-on;
 	};
-- 
2.20.1

