diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index bec8c4a..25d3be2 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -245,6 +258,24 @@
 				drive-strength = <40>;
 			};
 
+			i2c0_pins: i2c0 {
+				pins = "PD25", "PD26";
+				function = "i2c0";
+				pull = <1>;
+			};
+
+			i2c1_pins: i2c1 {
+				pins = "PH5", "PH6";
+				function = "i2c1";
+				pull = <1>;
+			};
+
+			i2c2_pins: i2c2 {
+				pins = "PD23", "PD24";
+				function = "i2c2";
+				pull = <1>;
+			};
+
 			mmc0_pins: mmc0-pins {
 				pins = "PF0", "PF1", "PF2", "PF3",
 				       "PF4", "PF5";
@@ -268,6 +294,45 @@
 			};
 		};
 
+		i2c0: i2c@5002000 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x05002000 0x400>;
+			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C0>;
+			resets = <&ccu RST_BUS_I2C0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c1: i2c@5002400 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x05002400 0x400>;
+			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C1>;
+			resets = <&ccu RST_BUS_I2C1>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c2: i2c@5002800 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x05002800 0x400>;
+			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C2>;
+			resets = <&ccu RST_BUS_I2C2>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c2_pins>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		mmc0: mmc@4020000 {
 			compatible = "allwinner,sun50i-h6-mmc",
 				     "allwinner,sun50i-a64-mmc";
