From a740ecc40aa9df18fbfb12925c1b7600c043a3cd Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Thu, 10 May 2018 21:27:51 -0500
Subject: [PATCH 082/146] arm64: dts: allwinner: a64: Enable A64 timer
 workaround

As instability in the architectural timer has been observed on multiple
devices using this SoC, inluding the Pine64 and the Orange Pi Win,
enable the workaround in the SoC's device tree.

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 62b880f68d6a..73f7e69755f8 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -281,6 +281,7 @@
 
 	timer {
 		compatible = "arm,armv8-timer";
+		allwinner,sun50i-a64-unstable-timer;
 		interrupts = <GIC_PPI 13
 			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
 			     <GIC_PPI 14
-- 
2.17.1

