From ffba271ad470d7caa12ea5f3cd369bfc5b0038c5 Mon Sep 17 00:00:00 2001
From: wuweidong <625769020@qq.com>
Date: Wed, 4 Sep 2019 11:19:32 +0800
Subject: [PATCH] ARM: dts: sun8i-h3-nanopi: Add new board ZeroPi

---
 arch/arm/boot/dts/Makefile            |  1 +
 arch/arm/boot/dts/sun8i-h3-zeropi.dts | 82 +++++++++++++++++++++++++++
 drivers/char/sunxi_soc_info.c         |  6 +-
 3 files changed, 88 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm/boot/dts/sun8i-h3-zeropi.dts

diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index 9570f05d2a663..3f980b4cd32d9 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -927,4 +927,5 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h3-nanopi-r1.dtb \
 	sun8i-h3-nanopi-duo2.dtb \
+	sun8i-h3-zeropi.dtb \
 	sun8i-h3-orangepi-2.dtb \
 	sun8i-h3-orangepi-lite.dtb \
diff --git a/arch/arm/boot/dts/sun8i-h3-zeropi.dts b/arch/arm/boot/dts/sun8i-h3-zeropi.dts
new file mode 100644
index 0000000000000..4edee84316249
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h3-zeropi.dts
@@ -0,0 +1,100 @@
+/*
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "sun8i-h3-nanopi.dtsi"
+
+/ {
+	model = "FriendlyElec ZeroPi";
+	compatible = "friendlyarm,zeropi", "allwinner,sun8i-h3";
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gmac_power_pin_nanopi>;
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&pio {
+	gmac_power_pin_nanopi: gmac_power_pin@0 {
+		pins = "PD6";
+		function = "gpio_out";
+	};
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&usb_otg {
+	status = "okay";
+	dr_mode = "peripheral";
+};
+
+&usbphy {
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+};
+
\ No newline at end of file
