From 8a91463b53e778e876ca296882fd3285e02d129f Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Mon, 25 Dec 2017 22:05:19 +0100
Subject: [PATCH 66/82] WIP: Figure out how to use new bluetooth/OF driver
 binding for BT chip

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index 027c6a76627f..8bba9ccd2592 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -649,6 +649,16 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
 	status = "okay";
+
+/*
+	bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		//max-speed = <921600>;
+		shutdown-gpios = <&r_pio 0 4 GPIO_ACTIVE_HIGH>;
+		device-wakeup-gpios = <&pio 7 5 GPIO_ACTIVE_HIGH>;
+		//host-wakeup-gpios = <&r_pio 0 5 GPIO_ACTIVE_HIGH>;
+	};
+	*/
 };
 
 /* GPS NEO-6M */
-- 
2.20.1

