diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
index 5851a47a..c2f1baa2 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
@@ -50,4 +50,31 @@
 / {
 	model = "Xunlong Orange Pi Plus 2E";
 	compatible = "xunlong,orangepi-plus2e", "allwinner,sun8i-h3";
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		reg = <0>;
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
 };