diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus.dts
index 1238de25a..ba5238ef5 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus.dts
@@ -57,6 +57,27 @@
 		enable-active-high;
 		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
 	};
+
+	reg_sy8113b: gpio-regulator {
+		compatible = "regulator-gpio";
+		regulator-name = "vdd-cpux";
+		regulator-type = "voltage";
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1300000>;
+		regulator-ramp-delay = <50>; /* 4ms */
+
+		gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+		enable-active-high;
+		gpios-states = <0x1>;
+		states = <1100000 0x0
+			  1300000 0x1>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_sy8113b>;
 };
 
 &ehci0 {
