From 25be6ff78bebfd869a3be0017715f101bd75bb64 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Mon, 14 May 2018 01:19:06 +0200
Subject: [PATCH 15/82] arm64: dts: sun50i-h5: Enable cpufreq-dt on H5 CPU

Uses OPPs shared with H3.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
index 60fc84a1fb44..acd90f390e88 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -52,6 +52,9 @@
 			device_type = "cpu";
 			reg = <0>;
 			enable-method = "psci";
+			clocks = <&ccu CLK_CPUX>;
+			clock-names = "cpu";
+			operating-points-v2 = <&cpu0_opp_table>;
 			clock-frequency = <1200000000>;
 			#cooling-cells = <2>;
 			cooling-min-level = <0>;
@@ -63,6 +66,7 @@
 			device_type = "cpu";
 			reg = <1>;
 			enable-method = "psci";
+			operating-points-v2 = <&cpu0_opp_table>;
 			clock-frequency = <1200000000>;
 		};
 
@@ -71,6 +75,7 @@
 			device_type = "cpu";
 			reg = <2>;
 			enable-method = "psci";
+			operating-points-v2 = <&cpu0_opp_table>;
 			clock-frequency = <1200000000>;
 		};
 
@@ -79,6 +84,7 @@
 			device_type = "cpu";
 			reg = <3>;
 			enable-method = "psci";
+			operating-points-v2 = <&cpu0_opp_table>;
 			clock-frequency = <1200000000>;
 		};
 	};
-- 
2.20.1

