From 3bfe739a6da69c2a51dbd6d4288975bedaee04f8 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sat, 30 Jun 2018 07:58:15 +0200
Subject: [PATCH 71/82] ARM: dts: sun8i-a83t: Add missing clock properties to
 cpu nodes

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t.dtsi | 12 ++++++++++++
 1 file changed, 12 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index c09d8ee2f7c5..17371e0614e2 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -77,6 +77,8 @@
 		};
 
 		cpu@1 {
+			clocks = <&ccu CLK_C0CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
@@ -87,6 +89,8 @@
 		};
 
 		cpu@2 {
+			clocks = <&ccu CLK_C0CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
@@ -97,6 +101,8 @@
 		};
 
 		cpu@3 {
+			clocks = <&ccu CLK_C0CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
@@ -122,6 +128,8 @@
 		};
 
 		cpu@101 {
+			clocks = <&ccu CLK_C1CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
@@ -132,6 +140,8 @@
 		};
 
 		cpu@102 {
+			clocks = <&ccu CLK_C1CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
@@ -142,6 +152,8 @@
 		};
 
 		cpu@103 {
+			clocks = <&ccu CLK_C1CPUX>;
+			clock-names = "cpu";
 			compatible = "arm,cortex-a7";
 			clock-frequency = <1200000000>;
 			device_type = "cpu";
-- 
2.20.1

