diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
index 93b8dd6be..bf9b9af71 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
@@ -48,11 +48,19 @@
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
 
 / {
 	model = "Xunlong Orange Pi Prime";
 	compatible = "xunlong,orangepi-prime", "allwinner,sun50i-h5";
 
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
 	aliases {
 		ethernet0 = &emac;
 		serial0 = &uart0;
@@ -109,13 +117,6 @@
 		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
 	};
 
-	reg_vcc3v3: vcc3v3 {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc3v3";
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
-	};
-
 	reg_usb0_vbus: usb0-vbus {
 		compatible = "regulator-fixed";
 		regulator-name = "usb0-vbus";
@@ -132,6 +133,10 @@
 	};
 };
 
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpux>;
+};
+
 &codec {
 	allwinner,audio-routing =
 		"Line Out", "LINEOUT",
@@ -226,6 +231,30 @@
 &ohci3 {
 	status = "okay";
 };
+&r_i2c {
+	status = "okay";
+
+	reg_vdd_cpux: regulator@65 {
+		compatible = "silergy,sy8106a";
+		reg = <0x65>;
+		regulator-name = "vdd-cpux";
+		silergy,fixed-microvolt = <1200000>;
+		/*
+		 * The datasheet uses 1.1V as the minimum value of VDD-CPUX,
+		 * however both the Armbian DVFS table and the official one
+		 * have operating points with voltage under 1.1V, and both
+		 * DVFS table are known to work properly at the lowest
+		 * operating point.
+		 *
+		 * Use 1.0V as the minimum voltage instead.
+		 */
+		regulator-min-microvolt = <1000000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-ramp-delay = <200>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+};
 
 &uart0 {
 	pinctrl-names = "default";
