From 0f0c62c90fc072355b2118d118715492710b8735 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Wed, 8 Nov 2017 04:55:15 +0100
Subject: [PATCH 35/82] ARM: dts: sun8i-a83t-tbs-a711: Reduce camera IOVDD
 voltage

---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index 9a87ce651224..1a711a28f682 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -389,8 +389,8 @@
 };
 
 &reg_dldo3 {
-	regulator-min-microvolt = <2800000>;
-	regulator-max-microvolt = <2800000>;
+	regulator-min-microvolt = <2600000>;
+	regulator-max-microvolt = <2600000>;
 	regulator-name = "vdd-csi";
 };
 
-- 
2.20.1

