diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index e3d5a6c..0d3eef6 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -995,6 +995,7 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h2-plus-orangepi-r1.dtb \
 	sun8i-h2-plus-bananapi-m2-zero.dtb \
 	sun8i-h2-plus-orangepi-zero.dtb \
+	sun8i-h2-plus-sunvell-r69.dtb \
 	sun8i-h3-bananapi-m2-plus.dtb \
 	sun8i-h3-beelink-x2.dtb \
 	sun8i-h3-libretech-all-h3-cc.dtb \
diff --git a/arch/arm/boot/dts/sun8i-h2-plus-sunvell-r69.dts b/arch/arm/boot/dts/sun8i-h2-plus-sunvell-r69.dts
new file mode 100644
index 0000000..1adfb0c
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h2-plus-sunvell-r69.dts
@@ -0,0 +1,215 @@
+/*
+ * Based original Sunvell R69 FEX file (2018 <github.com/karabek>)
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun8i-h3.dtsi"
+#include "sunxi-common-regulators.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
+
+/ {
+	model = "Sunvell R69";
+	compatible = "sunvell,sunvell-r69", "allwinner,sun8i-h2-plus";
+
+	aliases {
+		serial0 = &uart0;
+		ethernet0 = &emac;
+		ethernet1 = &xr819;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+ 	connector {
+ 		compatible = "hdmi-connector";
+ 		type = "a";
+ 
+ 		port {
+ 			hdmi_con_in: endpoint {
+ 				remote-endpoint = <&hdmi_out_con>;
+ 			};
+ 		};
+ 	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr_led {
+			label = "sunvell-r69:blue:pwr";
+			gpios = <&pio 0 15 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+		};
+
+		status_led {
+			label = "sunvell-r69:red:status";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	reg_vcc_wifi: reg_vcc_wifi {
+		compatible = "regulator-fixed";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc-wifi";
+		gpio = <&r_pio 0 7 GPIO_ACTIVE_HIGH>;
+	        startup-delay-us = <70000>;
+		enable-active-high;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 0 GPIO_ACTIVE_LOW>;
+		post-power-on-delay-ms = <200>;
+	};
+};
+
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&ir {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ir_pins_a>;
+	status = "okay";
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>;
+	cd-inverted;
+	status = "okay";
+};
+
+&mmc1_pins {
+	bias-pull-up;
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	/* pinctrl-0 = <&mmc1_pins>;	*/
+	vmmc-supply = <&reg_vcc_wifi>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	/*
+	 * Explicitly define the sdio device, so that we can add an ethernet
+	 * alias for it (which e.g. makes u-boot set a mac-address).
+	 */
+	xr819: sdio_wifi@1 {
+		reg = <1>;
+		compatible = "xradio,xr819";
+		interrupt-parent = <&pio>;
+		interrupts = <0 11 IRQ_TYPE_EDGE_RISING>;
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&tcon0 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "host";		/* host -or- peripheral */
+	status = "okay";
+};
+
+&usbphy {
+	/* USB VBUS is always on */
+	status = "okay";
+};
