diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index 2be23d600957..afed6c0dea6f 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -1004,6 +1004,11 @@
 			interrupt-controller;
 			#interrupt-cells = <3>;
 
+			r_cir_pin: r-cir-pin {
+				pins = "PL12";
+				function = "s_cir_rx";
+			};
+
 			r_rsb_pins: r-rsb-pins {
 				pins = "PL0", "PL1";
 				function = "s_rsb";
